{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Bill of Materials-CamBox_RV1106"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Bill of Materials-CamBox_RV1106","index":0,"n_rows":136,"n_cols":6,"rows_kept":136,"cut":false,"hidden":false,"merged":[]}
["Comment","Description","Designator","Footprint","LibRef","Quantity"]
["5V","85dB Active Buzzer (Built-in Driving Circuit) Electromagnetic 3kHz Through Hole,D=9mm Buzzers ROHS","BZ1","BZ-9x5.5","HNB09A05",1]
["2.2uF-100V","2.2uF ±10% 100V Ceramic Capacitor X7R 1206","C1","CAPC_1206_N","TCC1206X7R225K101HT",1]
["100nF","100V 100nF X7R ±10% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C2, C19","CAPC_1206_N","CC1206KKX7R0BB104",2]
["10uF 100V","10uF 100V 63mA@120Hz ±20% SMD,D6.3xL5.4mm Aluminum Electrolytic Capacitors - SMD ROHS","C3, C21","SMD,D6.3xL5.4mm","RVT2A100M0605",2]
["2.2uF","2.2uF ±10% 6.3V X5R 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT RoHS","C4, C154","CAPC_0603_N","CL10A225KQ8NNNC",2]
["100nF/4/16V","16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C5, C12, C32, C34, C42, C50, C51, C52, C54, C56, C58, C60, C61, C62, C63, C64, C65, C66, C67, C68, C69, C72, C73, C74, C75, C76, C77, C78, C79, C80, C82, C84, C86, C87, C88, C89, C91, C93, C94, C96, C97, C98, C99, C100, C103, C104, C105, C108, C111, C113, C116, C118, C119, C120, C121, C124, C125, C126, C127, C128, C129, C130, C131, C135, C137, C144, C145, C148, C160, C168, C171, C172, C173, C178, C186, C189, C191, C192, C197","C0402","CC0402KRX7R7BB104",79]
["10uF - 16V","CAP CER 10uF 16V X5R 0805","C6, C8, C31, C55, C70, C71, C81, C83, C85, C90, C92, C95, C101, C107, C110, C112, C115, C117, C122, C123, C132, C136, C155, C185, C188, C190","CAPC_0805_N","C0805X5R106K160NT",26]
["33pF 50V","C0G 33pF 50V ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C7, C46, C47, C141, C149, C150, C151, C159","C0402","CL05C330JB5NNNC",8]
["100nF","50V 100nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C9, C22, C25, C36, C102, C106, C134, C156, C158, C174, C175, C176, C193, C194, C195","CAPC_0603_N","CC0603KRX7R9BB104",15]
["10uF 50V","10uF ±10% 50V Ceramic Capacitor X5R 1206","C10, C16, C18, C28, C30, C35, C38, C45","CAPC_1206_N","TCC1206X5R106K500HT",8]
["680pF-50V","680pF ±10% 50V Ceramic Capacitor X7R 0402","C11","C0402","FCC0402B681K500AT",1]
["470uF 16V","470uF ±20% 16V Aluminum Electrolytic Capacitors 2000hrs@105℃","C13","SMD-ALU-D8xL10.2mm","RVT1C471M0810",1]
["8.2nF/4/50V","8.2nF ±10% 50V Ceramic Capacitor X7R 0402","C14","C0402","CC0402KRX7R9BB822",1]
["1uF - 50V","CAP CER 1UF 50V X5R 0603","C15, C49, C57, C59, C139, C170","CAPC_0603_N","C0603X5R105K500NT",6]
["22pF/50V","22pF ±5% 50V Ceramic Capacitor NP0 0402","C17","C0402","CC0402JRNPO9BN220",1]
["47uF-25V","47uF ±20% 25V Aluminum Electrolytic Capacitors 2000hrs@125℃","C20, C40","SMD,D6.3xL5.4mm","RT1E470M0605",2]
["470nF","50V 470nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C23","CAPC_0603_N","CC0603KRX7R9BB474",1]
["560pF - 0603","560 pF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)","C24","CAPC_0603_N","CC0603KRX7R9BB561",1]
["75pF","50V 75pF NP0 ±5% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C26","CAPC_0603_N","CC0603JRNPO9BN750",1]
["56nF","50V 56nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C27","CAPC_0603_N","CC0603KRX7R9BB563",1]
["22pF-50V","22pF ±5% 50V Ceramic Capacitor NP0 0402","C29","C0402","CC0402JRNPO9BN220",1]
["22pF","22pF ±5% 50V Ceramic Capacitor NP0 0402","C37","CAPC_0603_N","CC0402JRNPO9BN220",1]
["100pF - 50V","CAP CER 100PF 50V X7R 0603","C39","CAPC_0603_N","C0603X7R101J500NT",1]
["10uF - 50V","CAP CER 10uF 50V X5R 1206","C41","CAPC_1206_N","C1206X5R106K500NT",1]
["100pF/4/50V","50V 100pF NP0 ±1% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C44, C133, C143, C147, C161, C162, C166, C167, C169","C0402","CC0402FRNPO9BN101",9]
["22uF - 6.3V","CAP CER 22UF 6.3V X5R 0603","C53","CAPC_0603_N","CL10A226MQ8NRNE",1]
["100uF 10V","100uF ±20% 10V Ceramic Capacitor X5R 1206","C140, C146, C179","CAPC_1206_N","HGC1206R5107M100NSPJ",3]
["4.7uF - 35V","4.7uF 35V ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","C157","C0603X5R475K350NT","C0603X5R475K350NT",1]
["0.1uF","CAP CER 0.1UF 50V X7R 0603","C165","CAPC_0603_N","C0603X7R104K500NT",1]
["4.7uF - 6.3V","CAP CER 4.7UF 6.3V X5R 0603","C196","CAPC_0603_N","C0603X5R475K6R3NT",1]
["GREEN","20mA 180mcd Colorless Transparent Lens 565nm~575nm -20℃~+85℃ Positive Stick Yellow-green 120° 50mW 2.4V 0603 LED Indication - Discrete ROH","D1, D21, D32, D36, D56","0603-GREEN","XL-1608SYGC-04",5]
["LM-AZ6118-01F","DFN1006-2 TVS Diodes ROHS","D2, D4, D42, D43","DFN1006P2X","LM-AZ6118-01F",4]
["10A","Diode Independent 60V 10A Surface Mount TO-277B","D3","To-277B","",1]
["ESD5Z5V0","Unidirectional 5V (Max) 6.2V 18.6V 9.4A SOD-523 TVS RoHs","D5, D19, D30","SOD-523","ESD5Z5V0",3]
["40V-3A","40V Independent 500mV@3A 3A SMA(DO-214AC) Schottky Diodes ROHS","D6","DIO-SMA","SS34A",1]
["WE05DGCF-B","3A@8/20us 23V 70W@8/20us 6V 5V DFN1006-2L TVS Diodes RoHS","D7, D35","DFN1006-2L","WE05DGCF-B",2]
["5.1V","DIODE ZENER 5.1V 500MW SOD123","D8","SOD123","MMSZ5231B-7-F",1]
["B72590D50H160","0402 Varistors ROHS","D9, D10, D12, D13, D23, D24, D25, D26, D27, D28, D29, D34","D0402","B72590D50H160",12]
["1KV-1A","DIODE GEN PURP 1KV 1A SMA","D20, D47, D48","DIO-SMA","M7",3]
["RED","20mA 225mcd Colorless Transparent Lens -20℃~+85℃ Positive Stick 620nm~630nm Red 120° 50mW 2.3V 0603 LED Indication - Discrete ROH","D22, D33","0603-RED","XL-1608SURC-06",2]
["YELLOW","LED YELLOW CLEAR 0603 SMD","D31","0603-YELLOW","150060YS75000",1]
["5V9.2V","TVS DIODE 5V 9.2V SOD123F","D39, D40, D41, D44, D45","SOD123","SMF5.0A",5]
["S10M","Independent Type 10A 1.1V@10A 1kV SMC(DO-214AB) Diodes - General Purpose ROHS","D52","SMC(DO-214AB)","S10M",1]
["SMF36A","Unidirectional 36V 40V 58.1V 3.4A SOD-123FL TVS RoHS","D53","SOD-123FL","SMF36A",1]
["60V-3A","DIODE SCHOTTKY 60V 3A SMAF","D54, D55","DIO-SMA","SS36F",2]
["5A","10mΩ ±25% 10Ω@100MHz 0603 Ferrite Beads and Chips RoHS","E1, E2, E3, E4, E5, E16, E22, E29, E30, E31, E32","0603","YI160808U100-5R0T",11]
["1K-1.5A","FERRITE BEAD 1 KOHM 0805 1.5A","E6, E15, E26, E27, E28, E33","0805","UPZ2012E102-1R5TF",6]
["60Ω","60Ω@100MHz 1 Line Ferrite Bead 0402 600mA 150mΩ","E7, E8, E9, E10, E11, E12, E13, E14, E17, E18, E19, E20, E21","FERRITE_0402","CBW100505U600T",13]
["","","H1","HEATSINK_40x40x8","HEATSINK",1]
["TH-0.8-0.5-M1.4","SMD SMT ROHS","H2","TH-0.8-0.5-M1.4","SPACER",1]
["9P Male","9P Male D-Sub Bend insert 2 3A -50℃~+105℃ Push-Pull D-Sub / VGA Connectors ROHS","J4","D-Sub-9P-Male","D-DMR009PM-D002",1]
["IPEX","1 Inner pin IPEX Board-End 1.25mm -40℃~+90℃ 3GHz 50Ω 2mm SMD Coaxial Connectors (RF) ROHS","J5, J7, J9","IPEX","KH-IPEX-K501-29",3]
["M6110-01","NANO SIM+TF /NANO SIM*2","J6","MUP-M6110-01","",1]
["HR911105A","RJ45Receptacle 1 WithLED Plugin Ethernet Connectors / Modular Connectors (RJ45 RJ11) ROHS","J10","RJ45","HR911105A",1]
["4P2.0","JUMP-2.0-4PIN-FM-TH","J11","JUMP_4PIN_2.0","JUMP-2.0-4PIN-FM-TH",1]
["2x6P","2mm 2mm 2 12P 2x6P -40℃~+105℃ 4.3mm Top 2A Square Hole Through Hole Through Hole,P=2mm Headers, Receptacles, Female Sockets RoHS","J14, J15, J16","2x6P, 2mm, TH, MALE","PM200V-12-12-H43",3]
["2P2.54","XH Header Male Pin 0.098\"(2.50mm) 2 Through Hole Wire To Board / Wire To Wire Connector RoHS","J17","XH2.54-2P-R","XH-2AW",1]
["C7802-02","Card Connector NANO SIM Hinged Lid Surface Mount","J23","MUP-C7802-02","",1]
["4P2.54","Pin Header 4 1 Straight，180degrees 2.54mm Through Hole,P=2.54mm Pin Header & Female Header RoHS","J24","HEADER_4PIN_2.54","A2541WV-4P",1]
["2P2.54","XH Header Male Pin 0.098\"(2.50mm) 2 Through Hole Wire To Board / Wire To Wire Connector RoHS","J26","XH2.54-2P-2.54","XH-2A",1]
["AS0BC21-S40BM-7H","67P Surface Mount, Right Angle SMD,P=0.5mm,Surface Mount,Right Angle Centronics Connectors RoHS","J28","AS0BC21S40BM7H","AS0BC21-S40BM-7H (RV1106-PCIE)",1]
["TS-1090S-AR02026","Without bracket 50mA 3.5mm 100000 Times 260gf 12V 3mm 2mm Round Button Standing paste SPST SMD Tactile Switches ROHS","K1","SW4-SMD","TS-1090S-AR02026",1]
["2.2uH 8A","8A 2.2uH ±20% 8.8A 12.5mΩ SMD,7x6.6mm Fixed Inductors RoHS","L1","IND-7X6.6","ZD0650-2R2M",1]
["6.8uH-6A","6A 6.8uH ±20% 39mΩ 10A SMD,7.1x6.6mm Fixed Inductors RoHS","L2","IND-7X6.6","PSPMAA0605H-6R8M-ANP",1]
["22uH 3.3A","3.3A 22uH ±20% 7A SMD,12.2x12.2mm Arrays, Signal Transformers RoHS","L3","IND-12.2x12.2","CDRCH12D78BNP-220MC",1]
["2.2uH 3.2A","3.2A 2.2uH 5.8A 34mΩ ±20% SMD,4x4mm Fixed Inductors RoHS","L4, L5, L6","IND-4x4","NR4030S2R2MT",3]
["2.2uH 2A","2A 2.2uH Magnetic Shielded Inductor ±20% 2A 60mΩ SMD,3x3mm Fixed Inductors RoHS","L7","IND-3x3","ZNR3015ST2R2M",1]
["47nH","700mA 47nH 160mΩ ±5% 0402 Fixed Inductors RoHS","L8","L0402","VHF100505HQ47NJT",1]
["68nH","180mA 68nH ±5% 1.4Ω 0402 Fixed Inductors RoHS","L9","L0402","VHF100505HQ68NJT",1]
["DLW21SN670SQ2L","CMC 400MA 2LN 67 OHM SMD","L10","FIL_DLW21SN670SQ2L","DLM0NSN900HY2D",1]
["XL-DZ304SURD/3","60mA Red Lens 615nm~635nm -20℃~+85℃ Red 50° 150mW 1.8V~2.2V DIP-6-2.54mm LED Indication - Discrete ROHS","LED1, LED2","DIP-6-2.54mm","XL-DZ304SURD/3",2]
["SIM65M-C","GNSS Module with GPS, GLONASS, BDS, Galileo, QZSS, High Sensitivity, Low Power Consumption","M2","SIM65M-C","SIM65M-C",1]
["2SK3018","N-Channel 30V 0.1A 0.35W Surface Mount SOT-23","Q1, Q2, Q5, Q6, Q7, Q8, Q9, Q10, Q11, Q42","SOT-23-3","2SK3018",10]
["CSD19538Q3A","100V 15A 49mΩ@10V,5A 2.8W 3.2V 1 N-Channel VSONP-8(3.1x3.1) MOSFETs ROHS","Q3","VSONP-8(3.1x3.1)","CSD19538Q3A",1]
["40V-0.2A","TRANS NPN 40V 0.2A SOT23","Q4, Q12, Q16, Q17, Q19, Q21, Q23, Q24, Q25, Q26, Q27, Q28, Q29, Q30, Q31, Q32, Q33, Q34, Q37, Q38, Q39","SOT-23-3","MMBT3904-TP",21]
["P-CH 30V 4.2A","MOSFET P-CH 30V 4.2A SOT-23","Q13","SOT-23-3","ASDM3401ZA-R",1]
["SI2333CDS","SOT-23-3 MOSFETs P-Chanel ROHS","Q20, Q35, Q36","SOT-23-3","SI2333CDS",3]
["LBSS139LT1G","50V 200mA 225mW 5.6Ω@2.75V,200mA 500mV 1 N-channel SOT-23 MOSFETs ROHS","Q22","SOT-23-3","LBSS139LT1G",1]
["40V-0.2A","TRANS NPN 40V 0.2A SOT23","Q41","SOT-23-132","MMBT3904-TP",1]
["1R","RES SMD 1 OHM 1% 1/10W 0603","R1","RESC_0603_N","RI0603L1R00FT",1]
["100K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS","R2, R27, R40, R44, R46, R114, R238, R240, R242","R0402","RC0402FR-07100KL",9]
["118K/4/1%","62.5mW 118kΩ 50V Thick Film Resistor ±100ppm/℃ ±0.5% 0402 Chip Resistor - Surface Mount RoHS","R3","R0402","RC0402DR-07118KL",1]
["68K","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 68kΩ 0402 Chip Resistor - Surface Mount ROHS","R4","R0402","RC0402FR-0768KL",1]
["1.1K","RES 1.1kΩ ±1% 62.5mW 0402","R5, R10","R0402","0402WGF1101TCE",2]
["10K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS","R6, R13, R16, R17, R18, R25, R31, R33, R34, R35, R36, R39, R49, R100, R113, R115, R116, R120, R140, R142, R147, R155, R164, R165, R185, R186, R187, R191, R192, R193, R194, R195, R198, R199, R201, R202, R205, R234, R250, R257","R0402","RC0402FR-0710KL",40]
["51.1K/4/1%","51.1kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R7","R0402","RC0402FR-0751K1L",1]
["12K/4/1%","12kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R8","R0402","RC0402FR-0712KL",1]
["1K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 1kΩ 0402 Chip Resistor - Surface Mount ROHS","R9, R53, R78, R83, R86, R90, R94, R95, R102, R111, R112, R149, R156, R188, R189, R190, R196, R204, R233, R249, R256, R263","R0402","RC0402FR-071KL",22]
["105K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 105kΩ 0402 Chip Resistor - Surface Mount ROHS","R11","R0402","RC0402FR-07105KL",1]
["52.3kΩ/4/1%","62.5mW 52.3kΩ 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R12","R0402","RC0402FR-0752K3L",1]
["84.5K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 84.5kΩ 0402 Chip Resistor - Surface Mount ROHS","R14","R0402","RC0402FR-0784K5L",1]
["100R/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 100Ω 0402 Chip Resistor - Surface Mount ROHS","R15, R104, R105, R152","R0402","RC0402FR-07100RL",4]
["21.5K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 21.5kΩ 0402 Chip Resistor - Surface Mount ROHS","R19","R0402","RC0402FR-0721K5L",1]
["1.91K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 1.91kΩ 0402 Chip Resistor - Surface Mount ROHS","R20","R0402","RC0402FR-071K91L",1]
["15mΩ","500mW Thin Film Resistor ±100ppm/℃ ±0.5% 15mΩ 1206 Chip Resistor - Surface Mount ROHS","R21","RESC_1206_N","PE1206DRF7W0R015L",1]
["34K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 34kΩ 0402 Chip Resistor - Surface Mount ROHS","R22","R0402","RC0402FR-0734KL",1]
["45.3K/4/1%","45.3kΩ ±1% 62.5mW 0402 Thick Film Resistor","R23","R0402","RC0402FR-0745K3L",1]
["10K","RES 10K OHM 1% 1/16W 0402","R24, R235","R0402","RC0603FR-0710KL, RI0603L1002FT",2]
["499K/4/1%","62.5mW 499kΩ 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R26, R241","R0402","RC0402FR-07499KL",2]
["0R","100mW 0Ω 75V Thick Film Resistor ±5% 0603 Chip Resistor - Surface Mount RoHS, RES SMD 0 OHM JUMPER 1/10W 0603","R28, R30, R121, R127, R168","RESC_0603_N","RC0603JR-070RL, RI0603L000JT",5]
["8.45K/4/1%","8.45kΩ ±1% 62.5mW 0402 Thick Film Resistor","R29","R0402","RC0402FR-0745K3L",1]
["2.2K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 2.2kΩ 0402 Chip Resistor - Surface Mount ROHS","R32, R51, R52, R63, R71, R72, R76, R129, R130, R131, R208, R209, R210, R215, R216, R217, R255, R259","R0402","RC0402FR-072K2L",18]
["4.7K/4/1%","62.5mW Thick Film Resistors 50V ±100ppm/℃ ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS","R37, R38, R45, R64, R73, R80, R96, R97, R103, R134, R135, R141, R144, R148, R206, R211, R213, R218, R220, R221, R244, R251, R254, R260","R0402","RC0402FR-074K7L",24]
["22R/4/1%","50V Thick Film Resistors 62.5mW 22Ω ±1% ±100ppm/℃ 0402 Chip Resistor - Surface Mount ROHS","R41, R43, R47, R48, R60, R62, R69, R106, R107, R108, R109, R110, R124","R0402","RC0402FR-0722RL",13]
["1M/4/1%","62.5mW 1MΩ 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R42","R0402","RC0402FR-071ML",1]
["15K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 15kΩ 0402 Chip Resistor - Surface Mount ROHS","R50, R139","R0402","RC0402FR-0715KL",2]
["4.02K/4/0.1%","62.5mW 4.02Ω 50V Thick Film Resistor ±1% ±200ppm/℃ 0402 Chip Resistor - Surface Mount RoHS","R54","R0402","RC0402FR-074R02L",1]
["1.2K/4/1%","1.2kΩ ±1% 62.5mW 0402 Thick Film Resistor","R55","R0402","RC0402FR-071K2L",1]
["0Ω/4/1%","62.5mW 0Ω 50V ±1% Thick Film Resistors 0402 Chip Resistor - Surface Mount ROHS","R56, R57, R58, R59, R61, R65, R66, R67, R68, R70, R74, R75, R98, R99, R119, R128, R132, R138, R154, R157, R246, R247","R0402","RC0402FR-070RL",22]
["10R/4/1%","62.5mW Thick Film Resistor 50V ±1% ±200ppm/℃ 10Ω 0402 Chip Resistor - Surface Mount ROHS","R77, R81, R82, R85, R87, R88, R91, R92, R151, R253","R0402","RC0402FR-0710RL",10]
["75R/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 75Ω 0402 Chip Resistor - Surface Mount ROHS","R79, R84, R89, R93","R0402","RC0402FR-0775RL",4]
["220R/4/1%","220Ω 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R101","R0402","RC0402FR-07220RL",1]
["2.2Ω ±1%","62.5mW 2.2Ω 50V Thick Film Resistor ±1% ±200ppm/℃ 0402 Chip Resistor - Surface Mount RoHS","R122, R123, R125, R126","R0402","YAGEO RC0402FR-072R2L",4]
["47K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 47kΩ 0402 Chip Resistor - Surface Mount ROHS","R136, R137, R146, R150, R207, R212, R214, R219, R222, R223, R243, R245, R252, R258","R0402","RC0402FR-0747KL",14]
["470R/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 470Ω 0402 Chip Resistor - Surface Mount ROHS","R163","R0402","RC0402FR-07470RL",1]
["0R","RES 0 OHM 1206 JUMPER 1/4W SMD","R166","RESC_1206_N","RI1206L000JT",1]
["20K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 20kΩ 0402 Chip Resistor - Surface Mount ROHS","R171","R0402","RC0402FR-0720KL",1]
["590K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 590kΩ 0402 Chip Resistor - Surface Mount ROHS","R200","R0402","AC0402FR-07590KL",1]
["3.3K/4/1%","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 3.3kΩ 0402 Chip Resistor - Surface Mount ROHS","R203","R0402","RC0402FR-073K3L",1]
["10K 3435K","10kΩ ±1% 310uA 3435K 100mW ±1% 0603 NTC Thermistors ROHS","R236","RESC_0603_N","CMFA 103F3435",1]
["226k/4/1%","226kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R237","R0402","AC0402FR-07226KL",1]
["357K/4/1%","57kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","R239","R0402","RC0402FR-07357KL",1]
["LMR14050SDDAR","2.5MHz Buck Adjustable 800mV~28V 5A SOIC-8-EP Voltage Regulators - DC DC Switching Regulators RoHS","U1","8-POWERIC","LMR14050SDDAR",1]
["ETA3409S2F","Buck 1MHz Adjustable 600mV~7.3V 3A SOT23-5 Voltage Regulators - DC DC Switching Regulators RoHS","U2, U4, U7","SOT-23-5","ETA3409S2F",3]
["LM3481MMX/NOPB","IC REG CTRLR MULT TOP 10MSOP","U3","10-MSOP","LM3481MMX/NOPB",1]
["TLV75801PDBVR","500mA, low IQ, high precision, adjustable ultra-low dropout voltage regulator with enable function","U5, U8, U9, U10","SOT-23-5","TLV75801PDBVR",4]
["XS9922B","4Ch HD/SD Analog Video Decoder","U6","QFN-88(10x10mm)","XS9922B",1]
["SP3232","3V~5.5V SOP-16 Drivers, Receivers, Transceivers RoHS","U11, U14, U15","SOP16","SP3232AEIM/TR",3]
["A7677S","LTE CAT 1 module, 4G + (GNSS)","U12","A7677","A7670C-LNNV",1]
["SMF05CT1G-P","SOT-363-6 ESD and Surge Protection (TVS/ESD) ROHS","U18","SOT-363-6","SMF05CT1G-P",1]
["SR05-04A","SOT-26 ESD and Surge Protection (TVS/ESD) ROHS","U19","TSOT-23-6","SR05-04A",1]
["LM393DR","2mV 25nA Dual channel SOIC-8 Comparators ROHS","U21","SOIC-8","LM393DR",1]
["ETA6003Q3Q","2.5A, 3MHz Switching Charger with Dynamic Power Path Management","U22","ETA6003Q3Q-QFN16G-0.5-3X3MM","ETA6003Q3Q",1]
["R5F51405ADFM#10","RXv2 RX140 Microcontroller IC 32-Bit 48MHz 128KB (128K x 8) FLASH 64-LFQFP (10x10)","U23","QFP50P1200X1200X170-64N","R5F51405ADFM#10",1]
["27Mhz/20PF","Crystal 27MHz 10ppm 20pF 60Ω SMD2016-4P","X1","SMD2016-4P","2.D.1.270002002",1]