Protel Design System Design Rule Check
PCB File : E:\HARDWARE\GitDVD\MODUL_IO_ETEK\MODUL _IO\PCB.PcbDoc
Date     : 13/05/2026
Time     : 4:40:29 CH

ERROR : More than 500 violations detected, DRC was stopped

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
   Violation between Un-Routed Net Constraint: Net NetC11_1 Between Pad C11-1(-163.68mm,119.3mm) on Top Layer And Pad U1-5(-137.35mm,117.975mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C20-2(58.85mm,41.56mm) on Top Layer And Pad D15-1(64.088mm,13.35mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R46-2(51.7mm,35.495mm) on Top Layer And Pad C20-2(58.85mm,41.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C20-2(58.85mm,41.56mm) on Top Layer And Pad U3-5(58.85mm,43.3mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R58-1(107.293mm,124.7mm) on Top Layer And Pad C22-1(111.778mm,124.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC23_1 Between Pad Q2-3(27.85mm,-14.725mm) on Top Layer And Pad C23-1(29.875mm,-11.741mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U16-2(10mm,-11.875mm) on Multi-Layer And Pad C23-2(28.455mm,-11.741mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC24_1 Between Pad Q3-3(-156.434mm,95.902mm) on Top Layer And Pad C24-1(-154.189mm,98.115mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D6-1(-159.532mm,94.897mm) on Top Layer And Pad C24-2(-154.189mm,99.535mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C24-2(-154.189mm,99.535mm) on Top Layer And Pad U18-2(-133.441mm,80.586mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetC25_1 Between Pad Q4-3(-132.832mm,70.116mm) on Top Layer And Pad C25-1(-130.494mm,68.41mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D9-1(-135.836mm,65.192mm) on Top Layer And Pad C25-2(-130.494mm,69.83mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U18-2(-133.441mm,80.586mm) on Multi-Layer And Pad C25-2(-130.494mm,69.83mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC26_1 Between Pad U5-1(56.223mm,47.977mm) on Top Layer And Pad C26-1(300.688mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_9 Between Pad U5-2(56.223mm,49.247mm) on Top Layer And Pad C26-2(300.688mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC27_1 Between Pad R20-1(49.15mm,56.17mm) on Top Layer And Pad C27-1(284.088mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC27_1 Between Pad C27-1(284.088mm,10.19mm) on Top Layer And Pad U6-1(291.115mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_1 Between Pad J5-2(-159.625mm,108.075mm) on Multi-Layer And Pad C27-2(284.088mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_1 Between Pad C27-2(284.088mm,11.61mm) on Top Layer And Pad U6-2(291.115mm,10.203mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC28_1 Between Pad U5-3(56.223mm,50.517mm) on Top Layer And Pad C28-1(278.238mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_10 Between Track (54.4mm,48mm)(54.4mm,51.5mm) on Top Layer And Pad C28-2(278.238mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC29_1 Between Pad C29-1(272.388mm,10.19mm) on Top Layer And Pad U6-3(291.115mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC29_1 Between Via (38.594mm,64.7mm) from Top Layer to Bottom Layer And Pad C29-1(272.388mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_2 Between Pad J8-1(-144.385mm,108.075mm) on Multi-Layer And Pad C29-2(272.388mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_2 Between Pad C29-2(272.388mm,11.61mm) on Top Layer And Pad U6-4(291.115mm,7.663mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC30_1 Between Pad U5-5(56.223mm,53.057mm) on Top Layer And Pad C30-1(266.538mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_11 Between Pad U5-6(56.223mm,54.327mm) on Top Layer And Pad C30-2(266.538mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R40-1(45.719mm,44.9mm) on Top Layer And Pad C31-1(47.55mm,37.76mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C31-1(47.55mm,37.76mm) on Top Layer And Pad R46-2(51.7mm,35.495mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC32_1 Between Pad Q5-3(-140.613mm,34.067mm) on Top Layer And Pad C32-1(-140.327mm,36.405mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C32-2(-138.907mm,36.405mm) on Top Layer And Pad D10-1(-135.689mm,31.062mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C32-2(-138.907mm,36.405mm) on Top Layer And Pad D9-1(-135.836mm,65.192mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U19-2(-150.3mm,33.55mm) on Multi-Layer And Pad C32-2(-138.907mm,36.405mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC33_1 Between Pad C33-1(-120.868mm,26.79mm) on Top Layer And Pad Q6-3(-90.391mm,35.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC33_1 Between Pad C33-1(-120.868mm,26.79mm) on Top Layer And Pad U20-5(-109.752mm,10.691mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C33-2(-120.868mm,28.21mm) on Top Layer And Pad C34-2(-114.161mm,28.21mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D10-1(-135.689mm,31.062mm) on Top Layer And Pad C33-2(-120.868mm,28.21mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC34_1 Between Pad C34-1(-114.161mm,26.79mm) on Top Layer And Pad Q7-3(-84.014mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C34-2(-114.161mm,28.21mm) on Top Layer And Pad U20-2(-109.752mm,18.311mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetC35_1 Between Pad R24-1(51.65mm,88.08mm) on Top Layer And Pad C35-1(254.838mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC35_1 Between Pad C35-1(254.838mm,10.19mm) on Top Layer And Pad U6-5(291.115mm,6.393mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_3 Between Pad J8-2(-149.465mm,108.075mm) on Multi-Layer And Pad C35-2(254.838mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_3 Between Pad C35-2(254.838mm,11.61mm) on Top Layer And Pad U6-6(291.115mm,5.123mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC36_1 Between Pad C36-1(248.988mm,10.19mm) on Top Layer And Pad R26-1(260.838mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC36_1 Between Via (56.95mm,55.65mm) from Top Layer to Bottom Layer And Pad C36-1(248.988mm,10.19mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_12 Between Pad U5-8(56.223mm,56.867mm) on Top Layer And Pad C36-2(248.988mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC37_1 Between Pad C37-1(237.288mm,10.19mm) on Top Layer And Pad R27-1(243.288mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_4 Between Pad J13-1(-134.225mm,108.075mm) on Multi-Layer And Pad C37-2(237.288mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_4 Between Pad C37-2(237.288mm,11.61mm) on Top Layer And Pad U6-8(291.115mm,2.583mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC38_1 Between Pad C38-1(151.288mm,10.19mm) on Top Layer And Pad R32-1(163.138mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_13 Between Pad J6-2(-98.665mm,108.075mm) on Multi-Layer And Pad C38-2(151.288mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_13 Between Pad C38-2(151.288mm,11.61mm) on Top Layer And Pad U7-2(180.765mm,10.203mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC39_1 Between Pad C39-1(145.438mm,10.19mm) on Top Layer And Pad R37-1(157.288mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_5 Between Pad J13-2(-139.305mm,108.075mm) on Multi-Layer And Pad C39-2(145.438mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_5 Between Pad C39-2(145.438mm,11.61mm) on Top Layer And Pad U8-2(170.015mm,10.203mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC40_1 Between Pad C40-1(127.888mm,10.19mm) on Top Layer And Pad R38-1(139.738mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_14 Between Pad J11-1(-83.425mm,108.075mm) on Multi-Layer And Pad C40-2(127.888mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_14 Between Pad C40-2(127.888mm,11.61mm) on Top Layer And Pad U7-4(180.765mm,7.663mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC41_1 Between Pad C41-1(122.528mm,11.65mm) on Top Layer And Pad R39-1(133.888mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_6 Between Pad J18-1(-124.065mm,108.075mm) on Multi-Layer And Pad C41-2(123.948mm,11.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_6 Between Pad C41-2(123.948mm,11.65mm) on Top Layer And Pad U8-4(170.015mm,7.663mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC42_1 Between Pad C42-1(104.988mm,10.19mm) on Top Layer And Pad R42-1(116.838mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_15 Between Pad J11-2(-88.505mm,108.075mm) on Multi-Layer And Pad C42-2(104.988mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_15 Between Pad C42-2(104.988mm,11.61mm) on Top Layer And Pad U7-6(180.765mm,5.123mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC43_1 Between Pad C43-1(99.138mm,10.19mm) on Top Layer And Pad R54-1(110.988mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_7 Between Pad J18-2(-129.145mm,108.075mm) on Multi-Layer And Pad C43-2(99.138mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_7 Between Pad C43-2(99.138mm,11.61mm) on Top Layer And Pad U8-6(170.015mm,5.123mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC44_1 Between Pad C44-1(81.538mm,10.19mm) on Top Layer And Pad R55-1(93.438mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_16 Between Pad J16-1(-73.265mm,108.075mm) on Multi-Layer And Pad C44-2(81.538mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_16 Between Pad C44-2(81.538mm,11.61mm) on Top Layer And Pad U7-8(180.765mm,2.583mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC45_1 Between Pad C45-1(75.688mm,10.19mm) on Top Layer And Pad R56-1(87.588mm,9.82mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_8 Between Pad J21-1(-113.905mm,108.075mm) on Multi-Layer And Pad C45-2(75.688mm,11.61mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_8 Between Pad C45-2(75.688mm,11.61mm) on Top Layer And Pad U8-8(170.015mm,2.583mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC46_1 Between Pad C46-1(184.588mm,25.14mm) on Top Layer And Pad R63-1(196.488mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_17 Between Pad J16-2(-78.345mm,108.075mm) on Multi-Layer And Pad C46-2(184.588mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_17 Between Pad C46-2(184.588mm,26.56mm) on Top Layer And Pad U9-2(209.165mm,25.153mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC47_1 Between Pad C47-1(190.438mm,25.14mm) on Top Layer And Pad R64-1(202.338mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_25 Between Pad J7-2(-37.705mm,108.075mm) on Multi-Layer And Pad C47-2(190.438mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_25 Between Pad C47-2(190.438mm,26.56mm) on Top Layer And Pad U10-2(219.915mm,25.153mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC48_1 Between Pad C48-1(161.188mm,25.14mm) on Top Layer And Pad R65-1(173.088mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_18 Between Pad J19-1(-63.105mm,108.075mm) on Multi-Layer And Pad C48-2(161.188mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_18 Between Pad C48-2(161.188mm,26.56mm) on Top Layer And Pad U9-4(209.165mm,22.613mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC49_1 Between Pad C49-1(167.038mm,25.14mm) on Top Layer And Pad R66-1(178.938mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_26 Between Pad J12-1(-22.465mm,108.075mm) on Multi-Layer And Pad C49-2(167.038mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_26 Between Pad C49-2(167.038mm,26.56mm) on Top Layer And Pad U10-4(219.915mm,22.613mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC50_1 Between Pad C50-1(149.488mm,25.14mm) on Top Layer And Pad R67-1(155.538mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_19 Between Pad J19-2(-68.185mm,108.075mm) on Multi-Layer And Pad C50-2(149.488mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_19 Between Pad C50-2(149.488mm,26.56mm) on Top Layer And Pad U9-6(209.165mm,20.073mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC51_1 Between Pad C51-1(138.328mm,26.6mm) on Top Layer And Pad R68-1(143.788mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_20 Between Pad J22-1(-52.945mm,108.075mm) on Multi-Layer And Pad C51-2(139.748mm,26.6mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_20 Between Pad C51-2(139.748mm,26.6mm) on Top Layer And Pad U9-8(209.165mm,17.533mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC52_1 Between Pad C52-1(98.538mm,25.14mm) on Top Layer And Pad R73-1(104.538mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_21 Between Pad J22-2(-58.025mm,108.075mm) on Multi-Layer And Pad C52-2(98.538mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_21 Between Pad C52-2(98.538mm,26.56mm) on Top Layer And Pad U12-2(111.365mm,25.153mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC53_1 Between Pad C53-1(86.838mm,25.14mm) on Top Layer And Pad R74-1(92.838mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_22 Between Pad J33-1(-42.785mm,108.075mm) on Multi-Layer And Pad C53-2(86.838mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_22 Between Pad C53-2(86.838mm,26.56mm) on Top Layer And Pad U12-4(111.365mm,22.613mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC54_1 Between Pad C54-1(75.088mm,25.14mm) on Top Layer And Pad R75-1(81.138mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_23 Between Pad J33-2(-47.865mm,108.075mm) on Multi-Layer And Pad C54-2(75.088mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_23 Between Pad C54-2(75.088mm,26.56mm) on Top Layer And Pad U12-6(111.365mm,20.073mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC55_1 Between Pad C55-1(63.388mm,25.14mm) on Top Layer And Pad R76-1(69.438mm,24.77mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_24 Between Pad J7-1(-32.625mm,108.075mm) on Multi-Layer And Pad C55-2(63.388mm,26.56mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_24 Between Pad C55-2(63.388mm,26.56mm) on Top Layer And Pad U12-8(111.365mm,17.533mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC56_1 Between Pad Q1-3(-1.414mm,84.742mm) on Top Layer And Pad C56-1(2.286mm,85.007mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC56_1 Between Pad U15-5(1.995mm,71.765mm) on Multi-Layer And Pad C56-1(2.286mm,85.007mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D4-1(-5.314mm,89.417mm) on Top Layer And Pad C56-2(2.286mm,86.427mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC57_1 Between Pad Q8-3(-77.638mm,35.425mm) on Top Layer And Pad C57-1(-33.675mm,26.74mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U24-2(-48.907mm,20.589mm) on Multi-Layer And Pad C57-2(-33.675mm,28.16mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC58_1 Between Pad C58-1(-73.918mm,26.965mm) on Top Layer And Pad Q9-3(-71.261mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC58_1 Between Pad C58-1(-73.918mm,26.965mm) on Top Layer And Pad U23-5(-61.991mm,12.969mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C58-2(-73.918mm,28.385mm) on Top Layer And Pad C59-2(-67.211mm,28.385mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U22-2(-75.075mm,20.589mm) on Multi-Layer And Pad C58-2(-73.918mm,28.385mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC59_1 Between Pad C59-1(-67.211mm,26.965mm) on Top Layer And Pad Q10-3(-64.884mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC59_1 Between Pad C59-1(-67.211mm,26.965mm) on Top Layer And Pad U24-5(-48.907mm,12.969mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C59-2(-67.211mm,28.385mm) on Top Layer And Pad D12-1(-65.937mm,63.45mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad C59-2(-67.211mm,28.385mm) on Top Layer And Pad U23-2(-61.991mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net MCU_P40_AN000 Between Pad D21-C(-128.8mm,116.45mm) on Top Layer And Pad C8-2(-122.215mm,116.225mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net MCU_P40_AN000 Between Pad C8-2(-122.215mm,116.225mm) on Top Layer And Pad D3-A(-118.425mm,117.725mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC32_1 Between Pad Q5-3(-140.613mm,34.067mm) on Top Layer And Pad D10-2(-140.088mm,31.062mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D11-1(-71.537mm,63.45mm) on Top Layer And Pad D12-1(-65.937mm,63.45mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D14-1(-77.137mm,63.45mm) on Top Layer And Pad D11-1(-71.537mm,63.45mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC33_1 Between Pad Q6-3(-90.391mm,35.925mm) on Top Layer And Pad D11-2(-71.537mm,67.85mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D12-1(-65.937mm,63.45mm) on Top Layer And Pad U15-2(-5.625mm,71.765mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetC34_1 Between Pad Q7-3(-84.014mm,35.425mm) on Top Layer And Pad D12-2(-65.937mm,67.85mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D13-1(-82.737mm,63.45mm) on Top Layer And Pad D14-1(-77.137mm,63.45mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC57_1 Between Pad D13-2(-82.737mm,67.85mm) on Top Layer And Pad Q8-3(-77.638mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC58_1 Between Pad D14-2(-77.137mm,67.85mm) on Top Layer And Pad Q9-3(-71.261mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D15-1(64.088mm,13.35mm) on Top Layer And Pad R111-1(120.843mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC59_1 Between Pad U24-5(-48.907mm,12.969mm) on Multi-Layer And Pad D15-2(64.088mm,17.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC6_2 Between Pad D22-C(-157.02mm,111.8mm) on Top Layer And Pad U1-8(-137.35mm,114.165mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad D24-1(60.702mm,-8.632mm) on Top Layer And Pad D26-2(65.088mm,2.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad D24-1(60.702mm,-8.632mm) on Top Layer And Pad J53-2(78.425mm,-6.225mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad J20-2(83.088mm,12.85mm) on Multi-Layer And Pad D25-2(87.038mm,2.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad J53-2(78.425mm,-6.225mm) on Multi-Layer And Pad D25-2(87.038mm,2.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Track (50.02mm,15.58mm)(50.05mm,15.55mm) on Bottom Layer And Pad D26-2(65.088mm,2.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetD1_C Between Pad L1-1(-162.546mm,1.85mm) on Top Layer And Pad D2-C(-113.35mm,117.35mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net MCU_P40_AN000 Between Pad D3-A(-118.425mm,117.725mm) on Top Layer And Pad U4-60(-90.5mm,82.812mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U15-2(-5.625mm,71.765mm) on Multi-Layer And Pad D4-1(-5.314mm,89.417mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad D5-1(13.525mm,5.775mm) on Top Layer And Pad E1-1(22.8mm,54.35mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U16-2(10mm,-11.875mm) on Multi-Layer And Pad D5-1(13.525mm,5.775mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC23_1 Between Pad D5-2(9.125mm,5.775mm) on Top Layer And Pad U16-5(17.62mm,-11.875mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetC24_1 Between Pad D6-2(-159.532mm,99.296mm) on Top Layer And Pad Q3-3(-156.434mm,95.902mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad R43-1(57mm,33.905mm) on Top Layer And Pad D8-1(57.157mm,26.878mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Track (50.02mm,15.58mm)(50.05mm,15.55mm) on Bottom Layer And Pad D8-1(57.157mm,26.878mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC25_1 Between Pad D9-2(-135.836mm,69.591mm) on Top Layer And Pad Q4-3(-132.832mm,70.116mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad E1-1(22.8mm,54.35mm) on Top Layer And Pad R40-1(45.719mm,44.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U15-2(-5.625mm,71.765mm) on Multi-Layer And Pad E1-1(22.8mm,54.35mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Vin Between Pad E5-2(-142.4mm,115.475mm) on Top Layer And Pad E3-1(-103.6mm,117.25mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetE3_2 Between Pad L1-2(-159.546mm,1.85mm) on Top Layer And Pad E3-2(-102mm,117.25mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Rx_Jig Between Via (31.9mm,60.15mm) from Top Layer to Bottom Layer And Pad J2-1(63.888mm,94.7mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_9 Between Pad J21-2(-118.985mm,108.075mm) on Multi-Layer And Pad U5-2(56.223mm,49.247mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_1 Between Pad J23-1(-137.5mm,-12.125mm) on Multi-Layer And Track (30.4mm,32.5mm)(30.4mm,34.461mm) on Bottom Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_2 Between Pad J23-2(-132.42mm,-12.125mm) on Multi-Layer And Pad U16-1(10mm,-14.415mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_1 Between Track (30.4mm,34.461mm)(30.989mm,35.05mm) on Bottom Layer And Pad J24-1(134.738mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_2 Between Pad U16-1(10mm,-14.415mm) on Multi-Layer And Pad J25-1(128.888mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_3 Between Pad J26-1(-127.34mm,-12.125mm) on Multi-Layer And Pad J27-1(110.738mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_3 Between Pad U17-1(-159.345mm,78.81mm) on Multi-Layer And Pad J26-1(-127.34mm,-12.125mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_4 Between Pad U18-1(-135.981mm,80.586mm) on Multi-Layer And Pad J26-2(-122.26mm,-12.125mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_4 Between Pad U18-1(-135.981mm,80.586mm) on Multi-Layer And Pad J28-1(99.038mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_5 Between Pad U19-1(-150.3mm,31.01mm) on Multi-Layer And Pad J29-1(-117.18mm,-12.125mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U19-4(-142.68mm,43.71mm) on Multi-Layer And Pad J29-2(-112.1mm,-12.125mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_5 Between Pad U19-1(-150.3mm,31.01mm) on Multi-Layer And Pad J30-1(80.938mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad J3-1(89.838mm,124.2mm) on Top Layer And Pad R59-2(104.533mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad R60-1(84.893mm,124.7mm) on Top Layer And Pad J3-1(89.838mm,124.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U16-4(17.62mm,-1.715mm) on Multi-Layer And Pad J31-1(75.588mm,47.75mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_10 Between Pad J32-1(-103.745mm,108.075mm) on Multi-Layer And Track (54.865mm,51.965mm)(56.121mm,51.965mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_11 Between Pad J32-2(-108.825mm,108.075mm) on Multi-Layer And Pad U5-6(56.223mm,54.327mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_6 Between Pad U20-1(-112.292mm,18.311mm) on Multi-Layer And Pad J34-1(-107.02mm,-12.125mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_7 Between Pad J34-2(-101.94mm,-12.125mm) on Multi-Layer And Pad U21-1(-90.699mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_6 Between Pad U20-1(-112.292mm,18.311mm) on Multi-Layer And Pad J35-1(110.088mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_7 Between Pad U21-1(-90.699mm,20.589mm) on Multi-Layer And Pad J36-1(105.738mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_8 Between Pad J37-1(-96.86mm,-12.125mm) on Multi-Layer And Pad U22-1(-77.615mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_9 Between Pad J37-2(-91.78mm,-12.125mm) on Multi-Layer And Pad U23-1(-64.531mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_8 Between Pad U22-1(-77.615mm,20.589mm) on Multi-Layer And Pad J38-1(89.138mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_9 Between Pad U23-1(-64.531mm,20.589mm) on Multi-Layer And Pad J39-1(84.838mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_10 Between Pad J40-1(-86.7mm,-12.125mm) on Multi-Layer And Pad U24-1(-51.447mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad J40-2(-81.62mm,-12.125mm) on Multi-Layer And Pad U21-4(-77.999mm,12.969mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_10 Between Pad U24-1(-51.447mm,20.589mm) on Multi-Layer And Pad J41-1(68.188mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U24-3(-38.747mm,20.589mm) on Multi-Layer And Pad J42-1(63.888mm,21.9mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI_NPN_12 Between Pad J6-1(-93.585mm,108.075mm) on Multi-Layer And Pad U5-8(56.223mm,56.867mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Rx_Jig Between Pad U4-32(-79.1mm,88.312mm) on Top Layer And Pad J9-1(29.15mm,60.65mm) on Bottom Layer 
   Violation between Un-Routed Net Constraint: Net NetQ10_1 Between Pad R95-1(-119.776mm,41.73mm) on Top Layer And Pad Q10-1(-65.834mm,32.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ1_1 Between Pad R79-1(-0.613mm,89.317mm) on Top Layer And Pad Q1-1(-0.464mm,87.242mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC56_1 Between Track (-5.314mm,85.017mm)(-5.039mm,84.742mm) on Top Layer And Pad Q1-3(-1.414mm,84.742mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ2_1 Between Pad R78-1(29.92mm,-9.925mm) on Top Layer And Pad Q2-1(30.35mm,-15.675mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC23_1 Between Pad U16-5(17.62mm,-11.875mm) on Multi-Layer And Pad Q2-3(27.85mm,-14.725mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ3_1 Between Pad Q3-1(-155.484mm,98.402mm) on Top Layer And Pad R81-1(-152.567mm,98.106mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC24_1 Between Pad Q3-3(-156.434mm,95.902mm) on Top Layer And Pad U17-5(-151.725mm,81.35mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetQ4_1 Between Pad Q4-1(-133.782mm,67.616mm) on Top Layer And Pad R82-1(-128.871mm,68.401mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC25_1 Between Pad U18-5(-133.441mm,72.966mm) on Multi-Layer And Pad Q4-3(-132.832mm,70.116mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ5_1 Between Pad R85-1(-138.898mm,38.027mm) on Top Layer And Pad Q5-1(-138.113mm,33.117mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC32_1 Between Pad U19-5(-142.68mm,33.55mm) on Multi-Layer And Pad Q5-3(-140.613mm,34.067mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ6_1 Between Pad Q6-1(-91.341mm,33.425mm) on Top Layer And Pad R87-1(-68.709mm,41.73mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ7_1 Between Pad Q7-1(-84.964mm,32.925mm) on Top Layer And Pad R88-1(-61.414mm,41.73mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC34_1 Between Pad U21-5(-88.159mm,12.969mm) on Multi-Layer And Pad Q7-3(-84.014mm,35.425mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ8_1 Between Pad R91-1(-83.3mm,43.32mm) on Top Layer And Pad Q8-1(-78.588mm,32.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC57_1 Between Pad Q8-3(-77.638mm,35.425mm) on Top Layer And Pad U22-5(-75.075mm,12.969mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net NetQ9_1 Between Pad R92-1(-76.004mm,41.73mm) on Top Layer And Pad Q9-1(-72.211mm,32.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit2 Between Pad U4-44(-86.55mm,90.238mm) on Top Layer And Pad R10-1(80.593mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R107-1(238.043mm,26.65mm) on Top Layer And Pad R108-1(242.343mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R72-1(233.693mm,26.65mm) on Top Layer And Pad R107-1(238.043mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI19 Between Pad U9-12(215.475mm,21.343mm) on Top Layer And Pad R107-2(239.633mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R108-1(242.343mm,26.65mm) on Top Layer And Pad R109-1(246.693mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI20 Between Pad U9-10(215.475mm,18.803mm) on Top Layer And Pad R108-2(243.933mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R109-1(246.693mm,26.65mm) on Top Layer And Pad R110-1(251.043mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI25 Between Pad U10-16(226.225mm,26.423mm) on Top Layer And Pad R109-2(248.283mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R110-1(251.043mm,26.65mm) on Top Layer And Pad R31-1(306.393mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI26 Between Pad U10-14(226.225mm,23.883mm) on Top Layer And Pad R110-2(252.633mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net WDI_MCU Between Pad R11-1(55.4mm,43.305mm) on Top Layer And Track (56.945mm,43.305mm)(56.95mm,43.3mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net WDI_MCU Between Via (43.595mm,53.955mm) from Top Layer to Bottom Layer And Pad R11-1(55.4mm,43.305mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R111-1(120.843mm,26.65mm) on Top Layer And Pad R112-1(125.193mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI21 Between Pad U12-16(117.675mm,26.423mm) on Top Layer And Pad R111-2(122.433mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R112-1(125.193mm,26.65mm) on Top Layer And Pad R113-1(129.493mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI22 Between Pad U12-14(117.675mm,23.883mm) on Top Layer And Pad R112-2(126.783mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R113-1(129.493mm,26.65mm) on Top Layer And Pad R114-1(133.843mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI23 Between Pad U12-12(117.675mm,21.343mm) on Top Layer And Pad R113-2(131.083mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R114-1(133.843mm,26.65mm) on Top Layer And Pad R36-1(190.193mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI24 Between Pad U12-10(117.675mm,18.803mm) on Top Layer And Pad R114-2(135.433mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit3 Between Pad U4-39(-84.05mm,90.238mm) on Top Layer And Pad R12-1(76.243mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit4 Between Pad U4-37(-83.05mm,90.238mm) on Top Layer And Pad R13-1(71.943mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC26_1 Between Pad R14-1(23.25mm,45.72mm) on Top Layer And Pad U5-1(56.223mm,47.977mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit5 Between Pad U4-36(-82.55mm,90.238mm) on Top Layer And Pad R15-1(67.593mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit6 Between Pad U4-35(-82.05mm,90.238mm) on Top Layer And Pad R17-1(63.293mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit7 Between Pad U4-34(-81.55mm,90.238mm) on Top Layer And Pad R18-1(153.193mm,115.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit8 Between Pad U4-33(-81.05mm,90.238mm) on Top Layer And Pad R19-1(140.243mm,115.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC28_1 Between Pad R21-1(54.2mm,56.02mm) on Top Layer And Pad U5-3(56.223mm,50.517mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 24VDC_1 Between Pad R23-2(57.612mm,85.92mm) on Top Layer And Pad R22-2(59.3mm,85.92mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R25-1(323.743mm,11.7mm) on Top Layer And Pad R28-1(328.043mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R35-1(319.393mm,11.7mm) on Top Layer And Pad R25-1(323.743mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI9 Between Pad U5-16(49.913mm,47.977mm) on Top Layer And Pad R25-2(325.333mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC37_1 Between Pad R27-1(243.288mm,9.82mm) on Top Layer And Pad U6-7(291.115mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R28-1(328.043mm,11.7mm) on Top Layer And Pad R29-1(332.393mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI10 Between Pad U5-14(49.913mm,50.517mm) on Top Layer And Pad R28-2(329.633mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R29-1(332.393mm,11.7mm) on Top Layer And Pad R30-1(336.693mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI11 Between Pad U5-12(49.913mm,53.057mm) on Top Layer And Pad R29-2(333.983mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI12 Between Pad U5-10(49.913mm,55.597mm) on Top Layer And Pad R30-2(338.283mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R31-1(306.393mm,11.7mm) on Top Layer And Pad R33-1(310.743mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI1 Between Pad U6-16(297.425mm,11.473mm) on Top Layer And Pad R31-2(307.983mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC38_1 Between Pad R32-1(163.138mm,9.82mm) on Top Layer And Pad U7-1(180.765mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R33-1(310.743mm,11.7mm) on Top Layer And Pad R34-1(315.093mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI2 Between Pad U6-14(297.425mm,8.933mm) on Top Layer And Pad R33-2(312.333mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R34-1(315.093mm,11.7mm) on Top Layer And Pad R35-1(319.393mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI3 Between Pad U6-12(297.425mm,6.393mm) on Top Layer And Pad R34-2(316.683mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI4 Between Pad U6-10(297.425mm,3.853mm) on Top Layer And Pad R35-2(320.983mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R36-1(190.193mm,11.7mm) on Top Layer And Pad R48-1(194.543mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI5 Between Pad U8-16(176.325mm,11.473mm) on Top Layer And Pad R36-2(191.783mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC39_1 Between Pad R37-1(157.288mm,9.82mm) on Top Layer And Pad U8-1(170.015mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC40_1 Between Pad R38-1(139.738mm,9.82mm) on Top Layer And Pad U7-3(180.765mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC41_1 Between Pad R39-1(133.888mm,9.82mm) on Top Layer And Pad U8-3(170.015mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-RX Between Pad R40-2(44.129mm,44.9mm) on Top Layer And Pad U13-1(84.783mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad R41-2(55.35mm,33.905mm) on Top Layer And Pad R43-1(57mm,33.905mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC42_1 Between Pad R42-1(116.838mm,9.82mm) on Top Layer And Pad U7-5(180.765mm,6.393mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad R43-1(57mm,33.905mm) on Top Layer And Pad R61-1(80.593mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetR43_2 Between Pad R43-2(57mm,35.495mm) on Top Layer And Pad U13-7(86.053mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetR44_2 Between Pad R44-2(53.55mm,35.495mm) on Top Layer And Pad U13-6(87.323mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R48-1(194.543mm,11.7mm) on Top Layer And Pad R49-1(198.843mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI6 Between Pad U8-14(176.325mm,8.933mm) on Top Layer And Pad R48-2(196.133mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R49-1(198.843mm,11.7mm) on Top Layer And Pad R50-1(203.193mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI7 Between Pad U8-12(176.325mm,6.393mm) on Top Layer And Pad R49-2(200.433mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R50-1(203.193mm,11.7mm) on Top Layer And Pad R51-1(207.543mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI8 Between Pad U8-10(176.325mm,3.853mm) on Top Layer And Pad R50-2(204.783mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R51-1(207.543mm,11.7mm) on Top Layer And Pad R52-1(211.843mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI13 Between Pad U7-16(187.075mm,11.473mm) on Top Layer And Pad R51-2(209.133mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R52-1(211.843mm,11.7mm) on Top Layer And Pad R53-1(216.193mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI14 Between Pad U7-14(187.075mm,8.933mm) on Top Layer And Pad R52-2(213.433mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R53-1(216.193mm,11.7mm) on Top Layer And Pad R57-1(220.493mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI15 Between Pad U7-12(187.075mm,6.393mm) on Top Layer And Pad R53-2(217.783mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC43_1 Between Pad R54-1(110.988mm,9.82mm) on Top Layer And Pad U8-5(170.015mm,6.393mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC44_1 Between Pad R55-1(93.438mm,9.82mm) on Top Layer And Pad U7-7(180.765mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC45_1 Between Pad R56-1(87.588mm,9.82mm) on Top Layer And Pad U8-7(170.015mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R57-1(220.493mm,11.7mm) on Top Layer And Pad R71-1(229.393mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI16 Between Pad U7-10(187.075mm,3.853mm) on Top Layer And Pad R57-2(222.083mm,11.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R69-2(73.483mm,124.7mm) on Top Layer And Pad R58-1(107.293mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-RX Between Pad U14-1(78.283mm,84.845mm) on Top Layer And Pad R58-2(108.883mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Pad R61-1(80.593mm,124.7mm) on Top Layer And Pad R60-1(84.893mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetR60_2 Between Pad U14-7(79.553mm,90.255mm) on Top Layer And Pad R60-2(86.483mm,124.7mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetR62_2 Between Pad R62-2(77.833mm,124.7mm) on Top Layer And Pad U14-6(80.823mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC46_1 Between Pad R63-1(196.488mm,24.77mm) on Top Layer And Pad U9-1(209.165mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC47_1 Between Pad R64-1(202.338mm,24.77mm) on Top Layer And Pad U10-1(219.915mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC48_1 Between Pad R65-1(173.088mm,24.77mm) on Top Layer And Pad U9-3(209.165mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC49_1 Between Pad R66-1(178.938mm,24.77mm) on Top Layer And Pad U10-3(219.915mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC50_1 Between Pad R67-1(155.538mm,24.77mm) on Top Layer And Pad U9-5(209.165mm,21.343mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC51_1 Between Pad R68-1(143.788mm,24.77mm) on Top Layer And Pad U9-7(209.165mm,18.803mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R69-2(73.483mm,124.7mm) on Top Layer And Pad U14-8(78.283mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-DE Between Pad R70-1(67.593mm,124.7mm) on Top Layer And Pad U14-2(79.553mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit1 Between Pad U4-45(-87.05mm,90.238mm) on Top Layer And Pad R7-1(84.893mm,61.5mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad R71-1(229.393mm,26.65mm) on Top Layer And Pad R72-1(233.693mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI17 Between Pad U9-16(215.475mm,26.423mm) on Top Layer And Pad R71-2(230.983mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI18 Between Pad U9-14(215.475mm,23.883mm) on Top Layer And Pad R72-2(235.283mm,26.65mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC52_1 Between Pad R73-1(104.538mm,24.77mm) on Top Layer And Pad U12-1(111.365mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC53_1 Between Pad R74-1(92.838mm,24.77mm) on Top Layer And Pad U12-3(111.365mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC54_1 Between Pad R75-1(81.138mm,24.77mm) on Top Layer And Pad U12-5(111.365mm,21.343mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC55_1 Between Pad R76-1(69.438mm,24.77mm) on Top Layer And Pad U12-7(111.365mm,18.803mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ1_1 Between Pad R79-1(-0.613mm,89.317mm) on Top Layer And Pad R77-1(0.791mm,89.317mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ1_1 Between Pad R77-1(0.791mm,89.317mm) on Top Layer And Track (36.8mm,90mm)(37.055mm,89.745mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ2_1 Between Pad R80-1(25.445mm,-3.625mm) on Top Layer And Pad R78-1(29.92mm,-9.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO2 Between Pad R78-2(28.33mm,-9.925mm) on Top Layer And Pad U11-1(49.105mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ2_1 Between Pad R80-1(25.445mm,-3.625mm) on Top Layer And Track (36.85mm,85.65mm)(36.875mm,85.625mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ3_1 Between Pad R81-1(-152.567mm,98.106mm) on Top Layer And Pad R83-1(-150.995mm,98.106mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO3 Between Pad R81-2(-152.567mm,99.696mm) on Top Layer And Pad U11-2(50.375mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ4_1 Between Pad R82-1(-128.871mm,68.401mm) on Top Layer And Pad R84-1(-127.3mm,68.401mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO4 Between Pad R82-2(-128.871mm,69.991mm) on Top Layer And Pad U11-3(51.645mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ3_1 Between Pad R83-1(-150.995mm,98.106mm) on Top Layer And Track (23.25mm,45.855mm)(24.95mm,45.855mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ5_1 Between Pad R85-1(-138.898mm,38.027mm) on Top Layer And Pad R86-1(-138.898mm,39.599mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO5 Between Pad R85-2(-140.488mm,38.027mm) on Top Layer And Pad U11-4(52.915mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ6_1 Between Pad R87-1(-68.709mm,41.73mm) on Top Layer And Pad R89-1(-67.602mm,55.18mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO6 Between Pad R87-2(-68.709mm,43.32mm) on Top Layer And Pad U11-5(54.185mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ7_1 Between Pad R88-1(-61.414mm,41.73mm) on Top Layer And Pad R90-1(-60.619mm,55.18mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO7 Between Pad R88-2(-61.414mm,43.32mm) on Top Layer And Pad U11-6(55.455mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ8_1 Between Pad R93-1(-109.501mm,55.18mm) on Top Layer And Pad R91-1(-83.3mm,43.32mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO8 Between Pad R91-2(-83.3mm,41.73mm) on Top Layer And Pad U11-7(56.725mm,98.2mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ9_1 Between Pad R94-1(-95.535mm,55.18mm) on Top Layer And Pad R92-1(-76.004mm,41.73mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO9 Between Pad R92-2(-76.004mm,43.32mm) on Top Layer And Pad U2-15(101.188mm,53.825mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetQ10_1 Between Pad R96-1(-130.45mm,55.18mm) on Top Layer And Pad R95-1(-119.776mm,41.73mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO10 Between Pad R95-2(-119.776mm,43.32mm) on Top Layer And Pad U2-1(106.588mm,52.555mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit1 Between Pad SW1-1(-160.724mm,45.776mm) on Multi-Layer And Pad U4-45(-87.05mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit2 Between Pad SW1-2(-160.724mm,48.316mm) on Multi-Layer And Pad U4-44(-86.55mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit3 Between Pad SW1-3(-160.724mm,50.856mm) on Multi-Layer And Pad U4-39(-84.05mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit4 Between Pad SW1-4(-160.724mm,53.396mm) on Multi-Layer And Pad U4-37(-83.05mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit5 Between Pad SW1-5(-160.724mm,55.936mm) on Multi-Layer And Pad U4-36(-82.55mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit6 Between Pad SW1-6(-160.724mm,58.476mm) on Multi-Layer And Pad U4-35(-82.05mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit7 Between Pad SW1-7(-160.724mm,61.016mm) on Multi-Layer And Pad U4-34(-81.55mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net Bit8 Between Pad SW1-8(-160.724mm,63.556mm) on Multi-Layer And Pad U4-33(-81.05mm,90.238mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI26 Between Pad U4-46(-87.55mm,90.238mm) on Top Layer And Pad U10-14(226.225mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI25 Between Pad U4-47(-88.05mm,90.238mm) on Top Layer And Pad U10-16(226.225mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC6_1 Between Pad U1-1(-131.909mm,114.165mm) on Top Layer And Track (26.35mm,41.9mm)(26.35mm,41.925mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net GPIO1_3 Between Pad U4-25(-79.1mm,84.812mm) on Top Layer And Pad U11-11(55.455mm,103.6mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net GPIO1_2 Between Pad U4-26(-79.1mm,85.312mm) on Top Layer And Pad U11-12(54.185mm,103.6mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net GPIO1_1 Between Pad U4-27(-79.1mm,85.812mm) on Top Layer And Pad U11-14(51.645mm,103.6mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI24 Between Pad U4-48(-88.55mm,90.238mm) on Top Layer And Pad U12-10(117.675mm,18.803mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI23 Between Pad U4-49(-90.5mm,88.312mm) on Top Layer And Pad U12-12(117.675mm,21.343mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI22 Between Pad U4-50(-90.5mm,87.812mm) on Top Layer And Pad U12-14(117.675mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI21 Between Pad U4-51(-90.5mm,87.312mm) on Top Layer And Pad U12-16(117.675mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-DE Between Pad U13-2(86.053mm,84.845mm) on Top Layer And Pad U13-3(87.323mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-DE Between Via (28.15mm,55.2mm) from Top Layer to Bottom Layer And Pad U13-2(86.053mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-TX Between Pad U4-42(-85.55mm,90.238mm) on Top Layer And Pad U13-4(88.593mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U14-8(78.283mm,90.255mm) on Top Layer And Pad U13-8(84.783mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-RX Between Pad U4-14(-82.05mm,78.862mm) on Top Layer And Pad U14-1(78.283mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-DE Between Pad U14-2(79.553mm,84.845mm) on Top Layer And Pad U14-3(80.823mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-DE Between Pad U4-15(-81.55mm,78.862mm) on Top Layer And Pad U14-2(79.553mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-2-TX Between Pad U4-16(-81.05mm,78.862mm) on Top Layer And Pad U14-4(82.093mm,84.845mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U3-5(58.85mm,43.3mm) on Top Layer And Pad U14-8(78.283mm,90.255mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_NO_1 Between Pad U15-1(-5.625mm,69.225mm) on Multi-Layer And Track (30.4mm,32.5mm)(30.4mm,34.461mm) on Bottom Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U15-3(-5.625mm,81.925mm) on Multi-Layer And Pad U15-4(1.995mm,81.925mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U18-3(-123.281mm,80.586mm) on Multi-Layer And Pad U15-3(-5.625mm,81.925mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U15-4(1.995mm,81.925mm) on Multi-Layer And Pad U16-3(10mm,-1.715mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U16-3(10mm,-1.715mm) on Multi-Layer And Pad U16-4(17.62mm,-1.715mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U17-3(-159.345mm,91.51mm) on Multi-Layer And Pad U17-4(-151.725mm,91.51mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U17-4(-151.725mm,91.51mm) on Multi-Layer And Pad U18-3(-123.281mm,80.586mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U18-4(-123.281mm,72.966mm) on Multi-Layer And Pad U18-3(-123.281mm,80.586mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U19-4(-142.68mm,43.71mm) on Multi-Layer And Pad U18-4(-123.281mm,72.966mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_1 Between Pad U19-3(-150.3mm,43.71mm) on Multi-Layer And Pad U19-4(-142.68mm,43.71mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U20-2(-109.752mm,18.311mm) on Multi-Layer And Pad U21-2(-88.159mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U20-4(-99.592mm,10.691mm) on Multi-Layer And Pad U20-3(-99.592mm,18.311mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U20-3(-99.592mm,18.311mm) on Multi-Layer And Pad U21-3(-77.999mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net GPIO2_3 Between Pad U4-28(-79.1mm,86.312mm) on Top Layer And Pad U2-11(101.188mm,58.905mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net GPIO2_2 Between Pad U4-29(-79.1mm,86.812mm) on Top Layer And Pad U2-12(101.188mm,57.635mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U21-2(-88.159mm,20.589mm) on Multi-Layer And Pad U22-2(-75.075mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U21-4(-77.999mm,12.969mm) on Multi-Layer And Pad U21-3(-77.999mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U21-3(-77.999mm,20.589mm) on Multi-Layer And Pad U22-3(-64.915mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net GPIO2_1 Between Pad U4-30(-79.1mm,87.312mm) on Top Layer And Pad U2-14(101.188mm,55.095mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U22-4(-64.915mm,12.969mm) on Multi-Layer And Pad U22-3(-64.915mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U22-3(-64.915mm,20.589mm) on Multi-Layer And Pad U23-3(-51.831mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net 5V_VBUS Between Pad U23-2(-61.991mm,20.589mm) on Multi-Layer And Pad U24-2(-48.907mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U23-4(-51.831mm,12.969mm) on Multi-Layer And Pad U23-3(-51.831mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U23-3(-51.831mm,20.589mm) on Multi-Layer And Pad U24-3(-38.747mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DO_COM_6 Between Pad U24-4(-38.747mm,12.969mm) on Multi-Layer And Pad U24-3(-38.747mm,20.589mm) on Multi-Layer 
   Violation between Un-Routed Net Constraint: Net DI1 Between Pad U4-1(-88.55mm,78.862mm) on Top Layer And Via (30.151mm,49.251mm) from Top Layer to Bottom Layer 
   Violation between Un-Routed Net Constraint: Net DI2 Between Pad U4-11(-83.55mm,78.862mm) on Top Layer And Pad U6-14(297.425mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net WDI_MCU Between Pad U4-12(-83.05mm,78.862mm) on Top Layer And Via (43.595mm,53.955mm) from Top Layer to Bottom Layer 
   Violation between Un-Routed Net Constraint: Net DI3 Between Pad U4-13(-82.55mm,78.862mm) on Top Layer And Pad U6-12(297.425mm,6.393mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI4 Between Pad U4-17(-79.1mm,80.812mm) on Top Layer And Pad U6-10(297.425mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI5 Between Pad U4-18(-79.1mm,81.312mm) on Top Layer And Pad U8-16(176.325mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI6 Between Pad U4-19(-79.1mm,81.812mm) on Top Layer And Pad U8-14(176.325mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI8 Between Pad U4-20(-79.1mm,82.312mm) on Top Layer And Pad U8-10(176.325mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI9 Between Pad U4-21(-79.1mm,82.812mm) on Top Layer And Pad U5-16(49.913mm,47.977mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI10 Between Pad U4-22(-79.1mm,83.312mm) on Top Layer And Pad U5-14(49.913mm,50.517mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI11 Between Pad U4-23(-79.1mm,83.812mm) on Top Layer And Pad U5-12(49.913mm,53.057mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI12 Between Pad U4-24(-79.1mm,84.312mm) on Top Layer And Pad U5-10(49.913mm,55.597mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-DE Between Pad U4-41(-85.05mm,90.238mm) on Top Layer And Via (28.15mm,55.2mm) from Top Layer to Bottom Layer 
   Violation between Un-Routed Net Constraint: Net RS485-1-RX Between Pad U4-43(-86.05mm,90.238mm) on Top Layer And Track (28.817mm,54.15mm)(30.05mm,54.15mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI20 Between Pad U4-52(-90.5mm,86.812mm) on Top Layer And Pad U9-10(215.475mm,18.803mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI19 Between Pad U4-53(-90.5mm,86.312mm) on Top Layer And Pad U9-12(215.475mm,21.343mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI18 Between Pad U4-54(-90.5mm,85.812mm) on Top Layer And Pad U9-14(215.475mm,23.883mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI17 Between Pad U4-55(-90.5mm,85.312mm) on Top Layer And Pad U9-16(215.475mm,26.423mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI16 Between Pad U4-56(-90.5mm,84.812mm) on Top Layer And Pad U7-10(187.075mm,3.853mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI15 Between Pad U4-57(-90.5mm,84.312mm) on Top Layer And Pad U7-12(187.075mm,6.393mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI14 Between Pad U4-58(-90.5mm,83.812mm) on Top Layer And Pad U7-14(187.075mm,8.933mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI13 Between Pad U4-63(-90.5mm,81.312mm) on Top Layer And Pad U7-16(187.075mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net NetC30_1 Between Track (33.55mm,61.15mm)(33.55mm,62.35mm) on Top Layer And Pad U5-5(56.223mm,53.057mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net DI1 Between Via (30.151mm,49.251mm) from Top Layer to Bottom Layer And Pad U6-16(297.425mm,11.473mm) on Top Layer 
   Violation between Un-Routed Net Constraint: Net B1 Between Track (53.29mm,32.045mm)(53.41mm,32.165mm) on Top Layer And Track (55.283mm,33.838mm)(55.35mm,33.905mm) on Top Layer 
Rule Violations :392

Processing Rule : Modified Polygon (Allow modified: No), (Allow shelved: No)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.2mm) (Max=2mm) (Preferred=0.5mm) (All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All)
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=0.025mm) (Max=2.54mm) (All)
Rule Violations :0

Processing Rule : Hole To Hole Clearance (Gap=0.01mm) (All),(All)
Rule Violations :0

Processing Rule : Minimum Solder Mask Sliver (Gap=0.01mm) (All),(All)
Rule Violations :0

Processing Rule : Silk To Solder Mask (Clearance=0.01mm) (IsPad),(All)
Rule Violations :0

Processing Rule : Silk to Silk (Clearance=0.01mm) (All),(All)
Rule Violations :0

Processing Rule : Net Antennae (Tolerance=0mm) (All)
Rule Violations :0

Processing Rule : RoomDefinition (Bounding Region = (161.496mm, 92.175mm, 174.096mm, 115.918mm) (InComponentClass('Room Definition6'))
   Violation between Room Definition: Between DIP Component U15-Relay 5V-8P (-1.764mm,75.067mm) on Top Layer And RoomDefinition (Bounding Region = (161.496mm, 92.175mm, 174.096mm, 115.918mm) (InComponentClass('Room Definition6')) 
Rule Violations :1

Processing Rule : Room DO_4 (Bounding Region = (31.161mm, 89.475mm, 48.661mm, 108.5mm) (InComponentClass('Room Definition4'))
Rule Violations :0

Processing Rule : Room DO_5 (Bounding Region = (16.817mm, 53.949mm, 35.042mm, 71.449mm) (InComponentClass('Room Definition5'))
Rule Violations :0

Processing Rule : RoomDefinition_1 (Bounding Region = (177.1mm, 8.525mm, 200.575mm, 26.025mm) (InComponentClass('Room Definition3'))
   Violation between Room Definition: Between RoomDefinition_1 (Bounding Region = (177.1mm, 8.525mm, 200.575mm, 26.025mm) (InComponentClass('Room Definition3')) And SMT Small Component D5-6.2V (11.325mm,5.775mm) on Top Layer 
Rule Violations :1

Processing Rule : Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10'))
   Violation between Room Definition: Between DIP Component U20-Relay 5V-8P (-106.45mm,14.45mm) on Top Layer And Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) 
   Violation between Room Definition: Between DIP Component U21-Relay 5V-8P (-84.857mm,16.728mm) on Top Layer And Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) 
   Violation between Room Definition: Between DIP Component U22-Relay 5V-8P (-71.773mm,16.728mm) on Top Layer And Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) 
   Violation between Room Definition: Between DIP Component U23-Relay 5V-8P (-58.689mm,16.728mm) on Top Layer And Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) 
   Violation between Room Definition: Between DIP Component U24-Relay 5V-8P (-45.605mm,16.728mm) on Top Layer And Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And Small Component J34-2P-5.08 (-101.94mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And Small Component J37-2P-5.08 (-91.78mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And Small Component J40-2P-5.08 (-81.62mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component C33-0.1uF (-120.868mm,27.5mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component C34-0.1uF (-114.161mm,27.5mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component C57-0.1uF (-33.675mm,27.45mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component C58-0.1uF (-73.918mm,27.675mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component C59-0.1uF (-67.211mm,27.675mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component D11-6.2V (-71.537mm,65.65mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component D12-6.2V (-65.937mm,65.65mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component D13-6.2V (-82.737mm,65.65mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component D14-6.2V (-77.137mm,65.65mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component D15-6.2V (64.088mm,15.55mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J35-TP (110.088mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J36-TP (105.738mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J38-TP (89.138mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J39-TP (84.838mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J41-TP (68.188mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component J42-TP (63.888mm,21.9mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component Q10-40V-0.2A (-64.884mm,34.175mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component Q6-40V-0.2A (-90.391mm,34.675mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component Q7-40V-0.2A (-84.014mm,34.175mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component Q8-40V-0.2A (-77.638mm,34.175mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component Q9-40V-0.2A (-71.261mm,34.175mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R87-1K (-68.709mm,42.525mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R88-1K (-61.414mm,42.525mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R89-10K (-67.602mm,55.975mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R90-10K (-60.619mm,55.975mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R91-1K (-83.3mm,42.525mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R92-1K (-76.004mm,42.525mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R93-10K (-109.501mm,55.975mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R94-10K (-95.535mm,55.975mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R95-1K (-119.776mm,42.525mm) on Top Layer 
   Violation between Room Definition: Between Room DO6-10 (Bounding Region = (232mm, 78.45mm, 381.899mm, 97.25mm) (InComponentClass('DO6-10')) And SMT Small Component R96-10K (-130.45mm,55.975mm) on Top Layer 
Rule Violations :39

Processing Rule : Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5'))
   Violation between Room Definition: Between DIP Component U15-Relay 5V-8P (-1.764mm,75.067mm) on Top Layer And Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) 
   Violation between Room Definition: Between DIP Component U16-Relay 5V-8P (13.861mm,-8.573mm) on Top Layer And Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) 
   Violation between Room Definition: Between DIP Component U17-Relay 5V-8P (-155.484mm,84.652mm) on Top Layer And Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) 
   Violation between Room Definition: Between DIP Component U18-Relay 5V-8P (-130.139mm,76.725mm) on Top Layer And Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) 
   Violation between Room Definition: Between DIP Component U19-Relay 5V-8P (-146.439mm,36.852mm) on Top Layer And Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And Small Component J23-2P-5.08 (-132.42mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And Small Component J26-2P-5.08 (-122.26mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And Small Component J29-2P-5.08 (-112.1mm,-12.125mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component C23-0.1uF (29.165mm,-11.741mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component C24-0.1uF (-154.189mm,98.825mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component C25-0.1uF (-130.494mm,69.12mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component C32-0.1uF (-139.617mm,36.405mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component C56-0.1uF (2.286mm,85.717mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component D10-6.2V (-137.889mm,31.062mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component D5-6.2V (11.325mm,5.775mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component D6-6.2V (-159.532mm,97.097mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component D9-6.2V (-135.836mm,67.392mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component Q1-40V-0.2A (-1.414mm,85.992mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component Q2-40V-0.2A (29.1mm,-14.725mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component Q3-40V-0.2A (-156.434mm,97.152mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component Q4-40V-0.2A (-132.832mm,68.866mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component Q5-40V-0.2A (-139.363mm,34.067mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R77-1K (1.586mm,89.317mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R78-1K (29.125mm,-9.925mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R79-10K (-1.408mm,89.317mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R80-10K (24.65mm,-3.625mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R81-1K (-152.567mm,98.901mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R82-1K (-128.871mm,69.196mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R83-10K (-150.995mm,98.901mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R84-10K (-127.3mm,69.196mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R85-1K (-139.693mm,38.027mm) on Top Layer 
   Violation between Room Definition: Between Room DO1-5 (Bounding Region = (232mm, 56.8mm, 396.999mm, 77.15mm) (InComponentClass('DO1-5')) And SMT Small Component R86-10K (-139.693mm,39.599mm) on Top Layer 
Rule Violations :32

Processing Rule : Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2'))
   Violation between Room Definition: Between DIP Component U17-Relay 5V-8P (-155.484mm,84.652mm) on Top Layer And Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) 
   Violation between Room Definition: Between Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) And SMT Small Component C24-0.1uF (-154.189mm,98.825mm) on Top Layer 
   Violation between Room Definition: Between Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) And SMT Small Component D6-6.2V (-159.532mm,97.097mm) on Top Layer 
   Violation between Room Definition: Between Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) And SMT Small Component Q3-40V-0.2A (-156.434mm,97.152mm) on Top Layer 
   Violation between Room Definition: Between Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) And SMT Small Component R81-1K (-152.567mm,98.901mm) on Top Layer 
   Violation between Room Definition: Between Room DO_3 (Bounding Region = (7.666mm, 102.027mm, 25.166mm, 121.052mm) (InComponentClass('Room Definition2')) And SMT Small Component R83-10K (-150.995mm,98.901mm) on Top Layer 
Rule Violations :6

Processing Rule : Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU'))
   Violation between Room Definition: Between Component U3-APX823-26W5G-7 (57.9mm,44.65mm) on Top Layer And Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) 
   Violation between Room Definition: Between DIP Component SW1-SW-8bit (-164.534mm,54.666mm) on Top Layer And Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) 
   Violation between Room Definition: Between LCC Component U4-R5F51405ADFM#10 (-84.8mm,84.55mm) on Top Layer And Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component ANCHOR1-1mm (201.3mm,128.6mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component ANCHOR2-1mm (225.4mm,29.8mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C15-0.1uF (25.95mm,56.65mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C17-0.1uF (36.2mm,46.25mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C18-4.7uF - 6.3V (44.7mm,48.65mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C19-0.1uF (28.15mm,84.9mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C2-0.1uF (41mm,46.15mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C20-0.1uF (58.85mm,40.85mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component C5-0.1uF (38mm,46.3mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component E1-1K-1.5A (23.8mm,54.35mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component J10-TP (29.15mm,63.85mm) on Bottom Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component J9-TP (29.15mm,60.65mm) on Bottom Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R10-10K (81.388mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R11-1K (55.4mm,44.1mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R12-10K (77.038mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R13-10K (72.738mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R15-10K (68.388mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R16-4.7K (58.85mm,48.25mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R17-10K (64.088mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R18-10K (153.988mm,115.2mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R19-10K (141.038mm,115.2mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R7-10K (85.688mm,61.5mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R8-10K (28.4mm,91.1mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SMT Small Component R9-10K (28.15mm,83.2mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SOIC Component U11-74HC595 (53.55mm,100.9mm) on Top Layer 
   Violation between Room Definition: Between Room MCU (Bounding Region = (232.05mm, 118.55mm, 261.349mm, 153.6mm) (InComponentClass('MCU')) And SOIC Component U2-74HC595 (103.888mm,57mm) on Top Layer 
Rule Violations :29

Processing Rule : Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All)
Rule Violations :0


Violations Detected : 500
Waived Violations : 0
Time Elapsed        : 00:00:01