{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["GX Board"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GX Board","index":0,"n_rows":21,"n_cols":19,"rows_kept":21,"cut":false,"hidden":false,"merged":[[1,17,1,18],[2,17,2,18],[0,0,1,2],[0,3,0,8],[0,9,0,13],[1,3,1,8],[1,9,1,13],[2,0,2,1],[2,9,2,14],[20,4,20,15],[4,4,4,5],[4,6,4,7],[18,4,18,15],[19,4,19,15],[3,0,3,1],[3,9,3,14]]}
[null,null,null,{"$f":"UPPER(\"Bill of Materials\")","v":"BILL OF MATERIALS"},{"$nulls":5},"Rev:"]
[null,null,null,"GX-Board",{"$nulls":5},"Production QTY",{"$nulls":7},"BOM Export Date: 04/05/26 16:31:42"]
["Customer:",null,"Aithings","HW version:","5.0",null,"Checked by:",null,null,"Date created:",{"$nulls":7},"Website：https://www,lcsc,com/bom"]
["Board code:",null,"GX-Board","Prepared by:","Ducdv",null,"Approved by:",null,null,"26/03/2026"]
[]
["STT","Internal Code","Category","Description","Manufacturer","Partnumber","Manufacturer 2","Manufacturer's Part Number 2","Designator","QTY / Set","Production quantity","Total Quantity","Unit","Mounting type","Note","EXW Price\n(USD)","Total EXW Price\n(USD)","Supplier","Việc cần làm"]
[{"$f":"ROW(A7)-ROW($A$6)","v":1},null,"Capacitor","CAP CER 1UF 50V X5R 0603","FH","0603X105M500NT","Samsung Electro-Mechanics","CL10A105KB8NNNC","C1, C2, C3, C4",4,1000,{"$f":"J7*K7","v":4000},null,"SMD",null,null,{"$f":"P7*L7","v":0}]
[{"$f":"ROW(A8)-ROW($A$6)","v":2},null,"Connector","2x2P 4P Micro-Fit(MX 3,0) 3mm 2 2 3mm Direct Insert Plugin,P=3mm Wire To Board Connector ROHS","BOOMELE(Boom Precision Elec)","3.0-2*2A",null,null,"J7, J9, J10, J11, J12, J13",6,1000,{"$f":"J8*K8","v":6000},null,"SMD",null,null,{"$f":"P8*L8","v":0}]
[{"$f":"ROW(A9)-ROW($A$6)","v":3},null,"Connector","2x6P 12P Gold Brass -40℃~+105℃ Pin Header Black 2mm 2mm 250V 3A 2 2mm SMD,P=2mm Headers, Male Pins ROHS","XKB Connection","X4621WRS-2x06I-C40D64","XKB Connection","X4621WRS-2x03I-C40D64","J8, J14, J15",3,1000,{"$f":"J9*K9","v":3000},null,"SMD",null,null,{"$f":"P9*L9","v":0}]
[{"$f":"ROW(A10)-ROW($A$6)","v":4},null,"MOSFET","SOT-23-3 MOSFETs P-Chanel ROHS","TECH PUBLIC","SI2333CDS",null,null,"Q1, Q2, Q5, Q6",4,1000,{"$f":"J10*K10","v":4000},null,"SMD",null,null,{"$f":"P10*L10","v":0}]
[{"$f":"ROW(A11)-ROW($A$6)","v":5},null,"Resistor","62,5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS","FOJAN","FRC0402F1002TS","Yageo","RC0402FR-0710KL","R1, R2, R7, R8",4,1000,{"$f":"J11*K11","v":4000},null,"SMD",null,null,{"$f":"P11*L11","v":0}]
[{"$f":"ROW(A12)-ROW($A$6)","v":6},null,"Resistor","62,5mW Thick Film Resistors 50V ±100ppm/℃ ±1% 4,7kΩ 0402 Chip Resistor - Surface Mount ROHS","FOJAN","FRC0402F4701TS","Yageo","RC0402FR-074K7L","R3, R4, R9, R10",4,1000,{"$f":"J12*K12","v":4000},null,"SMD",null,null,{"$f":"P12*L12","v":0}]
[{"$f":"ROW(A13)-ROW($A$6)","v":7},null,"Resistor","62,5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 47kΩ 0402 Chip Resistor - Surface Mount ROHS","FOJAN","FRC0402F4702TS","Yageo","RC0402FR-0747KL","R5, R6, R11, R12",4,1000,{"$f":"J13*K13","v":4000},null,"SMD",null,null,{"$f":"P13*L13","v":0}]
[{"$f":"ROW(A14)-ROW($A$6)","v":8},null,"Transistor","TRANS NPN 60V 0,5A SOT23","TECH PUBLIC","TPMMBTA05","ON Semiconductor","MMBTA05LT1G","Q3, Q4, Q7, Q8",4,1000,{"$f":"J14*K14","v":4000},null,"SMD",null,null,{"$f":"P14*L14","v":0}]
[{"$f":"ROW(A15)-ROW($A$6)","v":9},null,"Connector","Giắc GX12-2P 2 Chân (Đực)","chxunda","XD-GX12-2P-F","LKTC","GX12-2P","J1",1,1000,{"$f":"J15*K15","v":1000},null,"TH",null,null,{"$f":"P15*L15","v":0}]
[{"$f":"ROW(A16)-ROW($A$6)","v":10},null,"Connector","Giắc GX12-4P 12mm 4 Chân (Đực)","chxunda","XD-GX12-4P-M","LKTC","GX12-4P","J2, J3, J5, J6",4,1000,{"$f":"J16*K16","v":4000},null,"TH",null,null,{"$f":"P16*L16","v":0}]
[{"$f":"ROW(A17)-ROW($A$6)","v":11},null,"PCB","PCB, 2 layer, 113,94 mm* 23,58 mm, PCB Thickness: 1,6mm, Gerber_Camerabox-gx_2025-11-24_Y2413","JLC","Y2413",null,null,null,1,1000,{"$f":"J17*K17","v":1000},null,"ASM",null,null,{"$f":"P17*L17","v":0}]
[{"$f":"ROW(A18)-ROW($A$6)","v":12},null,"Stencil",{"$nulls":6},1,1,{"$f":"J18*K18","v":1},null,"ASM",null,null,{"$f":"P18*L18","v":0}]
[{"$nulls":4},"TOTAL (USD):",{"$nulls":11},{"$f":"SUM(Q7:Q18)","v":0}]
[{"$nulls":4},"EXW Price / Board (USD):",{"$nulls":11},{"$f":"Q19/1000","v":0}]
[{"$nulls":4},"EXW Price / Board (VND):"]