Protel Design System Design Rule Check
PCB File : C:\Users\Windows 11\OneDrive\Fiducialx_Documents\_2Fiducial project\Cambox_v5.1_AIthings\_DesignFiles\CamBox_RV1106.PcbDoc
Date     : 6/8/2026
Time     : 10:19:51 AM

Processing Rule : Clearance Constraint (Gap=0.152mm) (InPolygon),(All)
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.508mm) (InPoly),(InNetClass('ETH') or InNetClass('ETH_2') or InNetClass('AHD1_CSI') or InNetClass('SDCard') or InNetClass('USB') or InNetClass('ANT') or InNetClass('ANT_GPS'))
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.152mm) (All),(InNetClass('All Nets'))
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.2mm) (InPolygon),(InPolygon)
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.152mm) (InNet('GND_EARTH')),(InNet('GND')or InNet('VBUS'))
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Modified Polygon (Allow modified: No), (Allow shelved: No)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.076mm) (Max=0.508mm) (Preferred=0.156mm) (InNetClass('ANT') or InNetClass('ANT_GPS') or InNetClass('SDCard') or InNetClass('USIM'))
Rule Violations :0

Processing Rule : Width Constraint (Min=0.2mm) (Max=0.508mm) (Preferred=0.254mm) (All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=0.152mm) (Conductor Width=0.254mm) (Air Gap=0.178mm) (Entries=4) (All)
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=0.152mm) (Max=5.08mm) (All)
Rule Violations :0

Processing Rule : Hole To Hole Clearance (Gap=0.254mm) (All),(All)
Rule Violations :0

Processing Rule : Minimum Solder Mask Sliver (Gap=0.01mm) (All),(All)
Rule Violations :0

Processing Rule : Silk To Solder Mask (Clearance=0.01mm) (IsPad),(All)
Rule Violations :0

Processing Rule : Silk to Silk (Clearance=0.01mm) (All),(All)
Rule Violations :0

Processing Rule : Net Antennae (Tolerance=0mm) (All)
Rule Violations :0

Processing Rule : Matched Lengths(Tolerance=0.254mm) (InxSignalClass('xCSI'))
Rule Violations :0

Processing Rule : Matched Lengths(Tolerance=0.254mm) (InNetClass('ETH') or InNetClass('ETH_2'))
Rule Violations :0

Processing Rule : Matched Lengths(Tolerance=0.127mm) (InxSignalClass('xCSI'))
Rule Violations :0

Processing Rule : Matched Lengths(Tolerance=0.127mm) (InxSignalClass('SDMCC'))
Rule Violations :0

Processing Rule : Matched Lengths(Tolerance=0.127mm) (InNetClass('USB'))
Rule Violations :0

Processing Rule : Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All)
Rule Violations :0


Violations Detected : 0
Waived Violations : 0
Time Elapsed        : 00:00:05