{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Field=VariantName"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Field=VariantName","index":0,"n_rows":60,"n_cols":13,"rows_kept":60,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[2,9,2,12],[3,9,3,12],[0,0,1,2],[0,3,0,8],[1,3,1,8],[0,9,0,11],[1,9,1,11]]}
[null,null,null,{"$f":"UPPER(\"Bill of Materials\")","v":"BILL OF MATERIALS"},{"$nulls":5},"Rev:"]
[null,null,null,"DRIVER IO",{"$nulls":5},"Production QTY"]
["Customer:",null,"White","HW version:","",null,"Checked by:",null,null,"Date created:"]
["Board code:",null,"White_Module","Prepared by:","Datnd",null,"Approved by:",null,null,"15/06/2026"]
["STT","Internal Code","Category","Description","Manufacture","Partnumber","Manufacturer 2","Manufacturer's Part Number 2","Designator","Quantity","Unit","Mounting type","Note"]
[{"$f":"ROW(A6)-ROW($A$5)","v":1},null,"Capacitor","100V 2.2uF X7R ±10% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","CCTC","CCTC TCC1206X7R225K101HT",null,null,"C1",1,null,"SMD"]
[2,null,"Capacitor","100V 100nF X7R ±10% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC1206KKX7R0BB104",null,null,"C2, C6",2,null,"SMD"]
[3,null,"Capacitor","10uF 100V 63mA@120Hz ±20% SMD,D6.3xL5.4mm Aluminum Electrolytic Capacitors - SMD ROHS","ROQANG","RVT2A100M0605",null,null,"C3",1,null,"SMD"]
[4,null,"Capacitor","50V 100nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603KRX7R9BB104",null,null,"C4, C5, C13, C19, C20, C21, C22, C24, C25, C26, C27, C28, C29, C30, C31, C32, C33, C34, C35, C36, C37, C38, C39, C40, C41, C42, C43, C44, C45, C47, C48, C49, C50, C51, C52, C53, C54, C55, C56, C57, C58, C59, C60, C61, C62, C63, C64, C65, C66, C67, C68, C69, C70, C71",54,null,"SMD"]
[5,null,"Capacitor","4.7uF ±10% 50V X5R 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT RoHS","Samsung Electro-Mechanics","CL21A475KBQNNNE",null,null,"C7, C8",2,null,"SMD"]
[6,null,"Capacitor","CAP CER 1000PF 25V X7R 0603","Walsin Technology Corporation","0603B102K250CT",null,null,"C9",1,null,"SMD"]
[7,null,"Capacitor","2.2uF ±10% 6.3V X5R 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT RoHS","Samsung Electro-Mechanics","CL10A225KQ8NNNC",null,null,"C10",1,null,"SMD"]
[8,null,"Capacitor","100uF 16V 22mΩ@100kHz ±20% 345mA@100kHz Plugin,D5xL11mm Aluminum Electrolytic Capacitors - Leaded ROHS","Rubycon","16ZLH100MEFC5X11",null,null,"C11, C12",2,null,"TH"]
[9,null,"Capacitor","CAP CER 0.015UF 25V C0G/NP0 0603","KEMET","C0603C153J3GAC7867",null,null,"C14",1,null,"SMD"]
[10,null,"Capacitor","CAP SAFETY 100pF ±10% 440V 400V TH",null,"CD45-B2GA101K-VKA",null,null,"C15",1,null,"TH"]
[11,null,"Capacitor","CAP CER 4.7uF 16V X5R 0805","Hottech","C0805X5R475K160NT",null,null,"C16, C17",2,null,"SMD"]
[12,null,"Capacitor","CAP CER 10uF 16V X5R 0805","Hottech","C0805X5R106K160NT",null,null,"C18",1,null,"SMD"]
[13,null,"Capacitor","CAP CER 4.7UF 6.3V X5R 0603","Hottech","C0603X5R475K6R3NT",null,null,"C23",1,null,"SMD"]
[14,null,"Capacitor","CAP CER 47NF 50V X7R 0603","Samsung Electro-Mechanics","CL10B473KB8VPJC",null,null,"C46",1,null,"SMD"]
[15,null,"Capacitor","CAP CER 330nF 25V X7R 0603","YAGEO","CC0603KRX7R8BB334",null,null,"C72, C73, C74",3,null,"SMD"]
[16,null,"Diode","Independent Type 10A 1.1V@10A 1kV SMC(DO-214AB) Diodes - General Purpose ROHS","GOODWORK","S10M",null,null,"D1",1,null,"SMD"]
[17,null,"Diode","Unidirectional 36V 40V 58.1V 3.4A SOD-123FL TVS RoHS","MDD(Microdiode Semiconductor)","SMF36A",null,null,"D2",1,null,"SMD"]
[18,null,"Diode","DFN1006-2 TVS Diodes ROHS","Leiditech","LM-AZ6118-01F",null,null,"D3, D4",2,null,"SMD"]
[19,null,"Diode","DIODE SCHOTTKY 60V 5A SMC","Diodes Incorporated","B560C-13-F",null,null,"D5",1,null,"SMD"]
[20,null,"Diode","31V, 19V Clamp 19A (8/20µs) Ipp Tvs Diode Surface Mount SOT-23-3","Littelfuse Inc.","SM712-02HTG",null,null,"D6, D9",2,null,"SMD"]
[21,null,"Diode","240V 150mA 5uA DO-214AA Thyristors (TSS) RoHS","BOURNS","TISP4240M3BJR-S2",null,null,"D7, D8, D10, D11, D12, D13",6,null,"SMD"]
[22,null,"Diode","Zener Diode Independent 6.2V 1W Surface Mount SMA(DO-214AC)","DIODES","SMAZ6V2-13-F",null,null,"D15, D16, D17, D18, D19, D20, D21, D22, D23, D24, D25, D26, D27, D28, D29",15,null,"SMD"]
[23,null,"Ferrite Bead","10mΩ ±25% 10Ω@100MHz 0603 Ferrite Beads and Chips RoHS","YJYCOIN","YI160808U100-5R0T",null,null,"E1, E2, E3",3,null,"SMD"]
[24,null,"Ferrite Bead","FERRITE BEAD 1 KOHM 0805 1.5A","Sunlord","UPZ2012E102-1R5TF",null,null,"E4",1,null,"SMD"]
[25,null,"Fuse","Polymeric PTC Resettable Fuse 60V 2A Surface Mount 2920","BHFUSE","BSMD2920-200-60V",null,null,"F1",1,null,"SMD"]
[26,null,"Connector","TERM BLK 2POS 3.81mm TH","Cixi Kefa Elec","KF128L-3.81-2P",null,null,"J1, J10, J11, J12, J13, J17",6,null,"TH"]
[27,null,"Connector","TERM BLK 3POS 3.81mm TH","Cixi Kefa Elec","KF128L-3.81-3P",null,null,"J4, J14, J15, J16",4,null,"TH"]
[28,null,"Connector","Jack Modular Connector RJ45 Through Hole, Right Angle Shielded","Ckmtw","R-RJ45R08P-B000",null,null,"J5",1,null,"SMD"]
[29,null,"Connector","TERM BLK 8POS 3.81mm TH","Cixi Kefa Elec","KF128L-3.81-8P",null,null,"J6, J7, J8, J9",4,null,"TH"]
[30,null,"Inductor","4A 2.2uH ±20% 6A SMD,4x4mm Power Inductors ROHS","Ceaiya","MAI4020S-2R2MT",null,null,"L1",1,null,"SMD"]
[31,null,"Inductor","4.5A 6.8uH ±20% 8A 45mΩ Magnetic Shielded Inductor SMD,7.3x6.6mm Fixed Inductors RoHS","Sunltech","SLO0630H6R8MTT",null,null,"L2, L3",2,null,"SMD"]
[{"$f":"ROW(A37)-ROW($A$5)","v":32},null,"LED","20mA 180mcd Colorless Transparent Lens 565nm~575nm -20℃~+85℃ Positive Stick Yellow-green 120° 50mW 2.4V 0603 LED Indication - Discrete ROH","XINGLIGHT","XL-1608SYGC-04",null,null,"LED_IN, LI1, LI2, LI3, LI4, LI5, LI6, LI7, LI8, LI9, LI10, LI11, LI12, LI13, LI14, LI15, LI16, LI17, LI18, LI19, LI20, LI21, LI22, LI23, LI24, LI25, LI26, LO1, LO2, LO3, LO4, LO5, LO6, LO7, LO8, LO9, LO10, LO11, LO12, LO13, LO14, LO15",42,null,"SMD"]
[33,null,"Transistor","TRANS NPN 40V 0.2A SOT23","Micro Commercial Co","MMBT3904-TP",null,null,"Q1, Q2, Q3, Q4, Q5, Q6, Q7, Q8, Q9, Q10, Q11, Q12, Q13, Q14, Q15",15,null,"SMD"]
[34,null,"Resistor","RES SMD 1 OHM 1% 1/10W 0603","Hottech","RI0603L1R00FT",null,null,"R1",1,null,"SMD"]
[35,null,"Resistor","100mW 100kΩ 75V Thick Film Resistor ±100ppm/℃ ±1% 0603 Chip Resistor - Surface Mount RoHS","YAGEO","RC0603FR-07100KL",null,null,"R2",1,null,"SMD"]
[36,null,"Resistor","100mW Thick Film Resistors 75V ±100ppm/℃ ±1% 15kΩ 0603 Chip Resistor - Surface Mount ROHS","Yageo","RC0603FR-0715KL",null,null,"R3",1,null,"SMD"]
[37,null,"Resistor","68kΩ 100mW 75V Thick Film Resistor ±100ppm/℃ ±1% 0603 Chip Resistor - Surface Mount RoHS","YAGEO","RC0603FR-0768KL",null,null,"R4",1,null,"SMD"]
[38,null,"Resistor","12kΩ 100mW 75V Thin Film Resistor ±50ppm/℃ ±0.1% 0603 Chip Resistor - Surface Mount RoHS","YAGEO","RT0603BRE0712KL",null,null,"R5",1,null,"SMD"]
[39,null,"Resistor","125mW 45.3kΩ 150V Thick Film Resistor ±100ppm/℃ ±1% 0805 Chip Resistor - Surface Mount RoHS","YAGEO","RC0805FR-0745K3L",null,null,"R6",1,null,"SMD"]
[40,null,"Resistor","RES SMD 10K OHM 1% 1/10W 0603","Yageo","RC0603FR-0710KL",null,null,"R7, R8, R9, R10, R11, R12, R21, R22, R23, R24, R25, R26, R27, R28, R37, R38, R39, R40, R41, R42, R43, R44, R75, R76, R77, R78, R79, R80, R85, R86, R87, R88, R91, R92, R95, R96, R98, R101, R102, R105, R106, R108, R111, R112, R115, R116, R118",47,null,"SMD"]
[41,null,"Resistor","RES SMD 2.2K OHM 1% 1/10W 0603","Hottech","RI0603L2201FT",null,null,"R13, R14, R15, R16, R17, R18, R19, R20, R29, R30, R31, R32, R33, R34, R35, R36",16,null,"SMD"]
[42,null,"Resistor","RES SMD 100 OHM 1% 1/10W 0603","Hottech","RI0603L1000FT",null,null,"R46, R49, R51, R54, R57, R59",6,null,"SMD"]
[43,null,"Resistor","RES SMD 10 OHM 1% 1/10W 0603","Yageo","RC0603FR-0710RL",null,null,"R47, R50, R55, R58",4,null,"SMD"]
[44,null,"Resistor","120Ω ±1% 0.1W ±100ppm/℃ 0603 Chip Resistor - Surface Mount RoHS","FH(Guangdong Fenghua Advanced Tech)","RS-03K1200FT",null,null,"R48, R56",2,null,"SMD"]
[45,null,"Resistor","RES SMD 4.7K OHM 1% 1/10W 0603","Hottech","RI0603L4701FT",null,null,"R61, R62",2,null,"SMD"]
[46,null,"Resistor","RES SMD 1K OHM 1% 1/10W 0603","Yageo, Hottech","RC0603FR-071KL, RI0603L1001FT",null,null,"R69, R70, R71, R72, R73, R74, R81, R82, R83, R84, R89, R90, R93, R94, R97, R99, R100, R103, R104, R107, R109, R110, R113, R114, R117, R119, R120, R121, R122, R123, R124, R125, R126, R127, R128, R129, R130, R131, R132, R133, R134, R135, R136, R137, R138, R139, R140, R141, R142, R143, R144, R145, R146, R147, R148, R149, R150, R151, R152, R153, R154, R155, R156, R157, R158, R159",66,null,"SMD"]
[47,null,"Switch","SMD-6P,7.2x7.2mm Rotary Switches RoHS","Khon","ES07MP-16RBZ-L1500",null,null,"S1",1,null,"SMD"]
[48,null,"IC","2.5MHz Step-down type Adjustable 800mV~50V 3A SO-8-EP Voltage Regulators - DC DC Switching Regulators RoHS","TI","LMR16030SDDAR",null,null,"U1",1,null,"SMD"]
[49,null,"IC","DC-DC modular power supply, 1W, fixed voltage input, isolated non-regulated single-channel output","EVISUN","B0505S-1WR3",null,null,"U2",1,null,"SMD"]
[50,null,"IC","IC SHIFT REGISTER 8BIT 16SOIC","Nexperia USA Inc.","74HC595D,118",null,null,"U3, U4",2,null,"SMD"]
[51,null,"IC","RXv2 RX140 Microcontroller IC 32-Bit 48MHz 128KB (128K x 8) FLASH 64-LFQFP (10x10)","RENESAS","R5F51405ADFM#10",null,null,"U5",1,null,"SMD"]
[52,null,"IC","16PIN ULTRA SMALL SSOP AC INPUT PHOTOTRANSISTOR PHOTOCOUPLER","Everlight Elec","ELQ3H4(TA)-G",null,null,"U6, U7, U8, U9, U12, U13, U14",7,null,"SMD"]
[53,null,"IC","256 Half-Duplex SOIC-16-300mil Drivers, Receivers, Transceivers RoHS","TI","ISO3082DW",null,null,"U10, U11",2,null,"SMD"]
[54,null,"IC","IC DRVR/RCVR MULTCH RS232 16SOIC","Texas Instruments","MAX3232CDR",null,null,"U15",1,null,"SMD"]
[55,null,"Relay","DIP,10.5x14.5mm Power Relays ROHS","Ningbo Keke New Era Appliance","HK4100F-DC5V-SHG",null,null,"U16, U17, U18, U19, U20, U21, U22, U23, U24, U25, U26, U27, U28, U29, U32",15,null,"TH"]