{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["RV1106_Board","GX Board","Vat_tu_phu","Chi phí"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RV1106_Board","index":0,"n_rows":146,"n_cols":27,"rows_kept":146,"cut":false,"hidden":false,"merged":[[3,0,3,1],[3,9,3,14],[0,0,1,2],[0,3,0,8],[0,9,0,13],[1,3,1,8],[1,9,1,13],[2,0,2,1],[2,9,2,14]]}
[null,null,null,{"$f":"UPPER(\"Bill of Materials\")","v":"BILL OF MATERIALS"},{"$nulls":5},"Rev:"]
[null,null,null,"Cambox_2026",{"$nulls":5},"Production QTY"]
["Customer:",null,"Aithings","HW version:","5.0",null,"Checked by:",null,null,"Date created:"]
["Board code:",null,"CameraBox","Prepared by:","Ducdv",null,"Approved by:",null,null,"08/05/2026"]
["STT","Internal Code","Category","Description","Manufacture","Partnumber","Manufacturer 2","Manufacturer's Part Number 2","Designator","Quantity","Sluong Board","Sluong cần","Unit","Mounting type","Note","Mrf#","Mfr.","Order Qty.","Unit Price(USD)","Ext.Price(USD)","LCSC#","Supplier"]
[{"$f":"ROW(A6)-ROW($A$5)","v":1},null,"Heat Sinks","HEAT SINK, BGA, 28.5 X 28.5 X 10",{"$nulls":4},"H1",1,10,{"$f":"J6*K6","v":10},{"$nulls":14},1]
[2,null,"Spacer","SMD SMT ROHS",null,"TH-0.8-0.5-M1.4",null,null,"H2",1,10,{"$f":"J7*K7","v":10},null,null,null,"-","-","-","-","-","-","-",{"$nulls":4},1]
[40,null,"SOM","PCIE-RV1106 PCIE","RONGPIN","PCIE-RV1106 PCIE",null,null,"SOM",1,10,10,null,"SMD",{"$nulls":7},"RONGPIN"]
[4,null,"IC","4Ch HD/SD Analog Video Decoder","CHIPUP","XS9922B",null,null,"U6",1,10,10,null,"ASM",null,"-","-","-","-","-","-","-",{"$nulls":4},1]
[5,null,"Capacitor","100V 2.2uF X7R ±10% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","CCTC","CCTC TCC1206X7R225K101HT",null,null,"C1",1,10,10,null,"SMD",null,"TCC1206X7R225K101HT","CCTC","10","0.0470",0.47,"C7393990","LCSC",{"$nulls":4},1]
[6,null,"Capacitor","100V 100nF X7R ±10% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC1206KKX7R0BB104",null,null,"C2, C19",2,10,20,null,"SMD",null,"CC1206KKX7R0BB104","YAGEO","50","0.0094",0.47,"C107181","LCSC",{"$nulls":4},1]
[7,null,"Capacitor","10uF 100V 63mA@120Hz ±20% SMD,D6.3xL5.4mm Aluminum Electrolytic Capacitors - SMD ROHS","ROQANG","RVT2A100M0605",null,null,"C3, C21",2,10,20,null,"SMD",null,"RVT2A100M0605","ROQANG","20","0.0234",0.47,"C5221839","LCSC",{"$nulls":4},"C3,C21"]
[8,null,"Capacitor","2.2uF ±10% 6.3V X5R 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT RoHS","\tSamsung Electro-Mechanics","CL10A225KQ8NNNC",null,null,"C4, C154",2,10,20,null,"SMD",null,"CL10A225KQ8NNNC","Samsung Electro-Mechanics","50","0.0040",0.2,"C71000","LCSC",{"$nulls":4},"C4"]
[9,null,"Capacitor","16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0402KRX7R7BB104",null,null,"C5, C12, C32, C34, C42, C50, C51, C52, C54, C56, C58, C60, C61, C62, C63, C64, C65, C66, C67, C68, C69, C72, C73, C74, C75, C76, C77, C78, C79, C80, C82, C84, C86, C87, C88, C89, C91, C93, C94, C96, C97, C98, C99, C100, C103, C104, C105, C108, C111, C113, C116, C118, C119, C120, C121, C124, C125, C126, C127, C128, C129, C130, C131, C135, C137, C144, C145, C148, C160, C168, C171, C172, C173, C178, C186, C189, C191, C192, C197",79,10,790,null,"SMD",null,"CC0402KRX7R7BB104","YAGEO","800","0.0006",0.48,"C60474","LCSC",{"$nulls":4},"C32,C191,C12,C34,C171,C104,C105,C192,C197,C5,58,56,60,61,62,72,73,74,75,76,77,79,82,"]
[10,null,"Capacitor","CAP CER 10uF 16V X5R 0805","Hottech","C0805X5R106K160NT",null,null,"C6, C8, C31, C55, C70, C71, C81, C83, C85, C90, C92, C95, C101, C107, C110, C112, C115, C117, C122, C123, C132, C136, C155, C185, C188, C190",26,10,260,null,"SMD",null,"0805X5R106K160NT","AIDE CAPACITOR",300,"-",4.5599999999999996,"-","LCSC",{"$nulls":4},"C31,C190,C8,C6"]
[11,null,"Capacitor","NP0 33pF 50V ±5% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603JRNPO9BN330",null,null,"C7",1,10,10,null,"SMD",null,"CC0603JRNPO9BN330","YAGEO","100","0.0015",0.15,"C107047","LCSC",{"$nulls":4},1]
[12,null,"Capacitor","50V 100nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603KRX7R9BB104",null,null,"C9, C22, C25, C36, C102, C106, C156, C158, C174, C175, C176, C193, C194, C195",14,10,140,null,"SMD",null,"CC0603KRX7R9BB104","YAGEO","200","0.0014",0.28000000000000003,"C14663","LCSC",{"$nulls":4},"C9,C25, C106, c193,c174,c194,c195, c175,C22"]
[13,null,"Capacitor","10uF 50V Ceramic Capacitor X7R 1210","SAMWHA","CS3225X7R106K500NRL",null,null,"C10,  C18, C28, C30, C38, C16, C35, C45",8,10,80,null,"SMD",null,"CS3225X7R106K500NRL","SAMWHA","80","0.0466",3.73,"C2918502","LCSC",{"$nulls":4},"c10,c28,c30,C38"]
[14,null,"Capacitor","680pF ±10% 50V Ceramic Capacitor X7R 0402","FOJAN, SAMWHA","FCC0402B681K500AT",null,null,"C11",1,10,10,null,"SMD",null,"FCC0402B681K500AT","FOJAN","100","0.0005",0.05,"C5137577","LCSC",{"$nulls":4},1]
[15,null,"Capacitor","470uF ±20% 16V Aluminum Electrolytic Capacitors 2000hrs@105℃","ROQANG","RVT1C471M0810",null,null,"C13",1,10,10,null,"SMD",null,"RVT1C471M0810","ROQANG","10","0.0515",0.52,"C72517","LCSC",{"$nulls":4},1]
[16,null,"Capacitor","8.2nF ±10% 50V Ceramic Capacitor X7R 0402","Yageo","CC0402KRX7R9BB822",null,null,"C14",1,10,10,null,"SMD",null,"CC0402KRX7R9BB822","YAGEO","100","0.0001",0.01,"C107032","LCSC",{"$nulls":4},1]
[17,null,"Capacitor","CAP CER 1UF 50V X5R 0603","Hottech","C0603X5R105K500NT",null,null,"C15, C48, C49, C57, C59, C139, C170",7,10,70,null,"SMD",null,"0603X5R105K500NT","AIDE CAPACITOR",100,"-",0.72,"-","LCSC",{"$nulls":4},"C15"]
[18,null,"Capacitor","22pF ±5% 50V Ceramic Capacitor NP0 0402","Yageo","CC0402JRNPO9BN220",null,null,"C17, C29,C37",3,10,30,null,"SMD",null,"CC0402JRNPO9BN220","YAGEO","100","0.0006",0.06,"C106203","LCSC",{"$nulls":4},1]
[19,null,"Capacitor","16V 47uF X5R ±20% 1206 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Taiyo Yuden","EMK316BBJ476ML-T",null,null,"C20, C179",2,10,20,null,"SMD",null,"EMK316BBJ476ML-T","Taiyo Yuden","20","0.0749",1.5,"C385907","LCSC",{"$nulls":4},"C179,C20"]
[20,null,"Capacitor","50V 470nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603KRX7R9BB474",null,null,"C23",1,10,10,null,"SMD",null,"CC0603KRX7R9BB474","YAGEO","50","0.0065",0.33,"C513577","LCSC",{"$nulls":4},1]
[21,null,"Capacitor","560 pF ±10% 50V Ceramic Capacitor X7R 0603 (1608 Metric)","Yageo","CC0603KRX7R9BB561",null,null,"C24",1,10,10,null,"SMD",null,"CC0603KRX7R9BB561","YAGEO","100","0.0015",0.15,"C107094","LCSC",{"$nulls":4},1]
[22,null,"Capacitor","50V 75pF NP0 ±5% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603JRNPO9BN750",null,null,"C26",1,10,10,null,"SMD",null,"CC0603JRNPO9BN750","YAGEO","100","0.0015",0.15,"C282074","LCSC",{"$nulls":4},1]
[23,null,"Capacitor","50V 56nF X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0603KRX7R9BB563",null,null,"C27",1,10,10,null,"SMD",null,"CC0603KRX7R9BB563","YAGEO","100","0.0015",0.15,"C282072","LCSC",{"$nulls":4},1]
[24,null,"Capacitor","CAP CER 100PF 50V X7R 0603","YAGEO","CC0603KRX7R9BB101",null,null,"C39",1,10,10,null,"SMD",null,"-","-","100","-",0.28000000000000003,"-","LCSC",{"$nulls":4},1]
[25,null,"Capacitor","100uF 50V 146mA@120Hz ±20% SMD,D8xL10.2mm Aluminum Electrolytic Capacitors - SMD ROHS","ROQANG","RT1H101M0810",null,null,"C40",1,10,10,null,"SMD",null,"RT1H101M0810","ROQANG","10","0.0523",0.52,"C280404","LCSC",{"$nulls":4},1]
[26,null,"Capacitor","CAP CER 10uF 50V X5R 1206","YAGEO","CC1206KKX5R9BB106",null,null,"C41",1,10,10,null,"SMD",null,"-","-",10,"-",0.66,"-","LCSC",{"$nulls":4},1]
[27,null,"Capacitor","50V 100pF NP0 ±1% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Yageo","CC0402FRNPO9BN101",null,null,"C44, C133, C143, C161, C162, C166, C167, C169",8,10,80,null,"SMD",null,"CC0402FRNPO9BN101","YAGEO","100","0.0016",0.16,"C327198","LCSC"]
[28,null,"Capacitor","C0G 33pF 50V ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","Samsung Electro-Mechanics","CL05C330JB5NNNC",null,null,"C46, C47, C149, C150, C151, C159",6,10,60,null,"SMD",null,"CL05C330JB5NNNC","Samsung Electro-Mechanics","100","0.0017",0.17,"C70465","LCSC"]
[29,null,"Capacitor","CAP CER 22UF 6.3V X5R 0603","Samsung Electro-Mechanics","CL10A226MQ8NRNE",null,null,"C53",1,10,10,null,"SMD",null,"CL10A226MQ8NRNE","Samsung Electro-Mechanics","20","0.0068",0.14000000000000001,"C159801","LCSC"]
[30,null,"Capacitor","100uF ±20% 16V Ceramic Capacitor X5R 1210","Taiyo Yuden","EMK325ABJ107MM-T",null,null,"C140, C146",2,10,20,null,"SMD",null,"EMK325ABJ107MM-T","Taiyo Yuden","20","0.2769",5.54,"C394395","LCSC"]
[31,null,"Capacitor","50V 33pF C0G ±5% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","FH(Guangdong Fenghua Advanced Tech)","0805CG330J500NT",null,null,"C141",1,10,10,null,"SMD",null,"0805CG330J500NT","FH","100","0.0025",0.25,"C157687","LCSC"]
[32,null,"Capacitor","50V 10pF C0G ±5% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","PSA(Prosperity Dielectrics)","FN21N100J500PAG",null,null,"C142",1,10,10,null,"SMD",null,"FN21N100J500PAG","PSA","100","0.0035",0.35,"C525280","LCSC"]
[33,null,"Capacitor","4.7uF 35V ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS","AIDE CAPACITOR","C0603X5R475K350NT",null,null,"C157",1,10,10,null,"SMD",null,"-","-",20,"-",0.62,"-","LCSC"]
[34,null,"Capacitor","CAP CER 0.1UF 50V X7R 0603","AIDE CAPACITOR","C0603X7R104K500NT",null,null,"C165",1,10,10,null,"SMD",null,"-","-","100","-",0.25,"-","LCSC"]
[35,null,"Capacitor","CAP CER 4.7UF 6.3V X5R 0603","AIDE CAPACITOR","C0603X5R475K6R3NT",null,null,"C196",1,10,10,null,"SMD",null,"-","-","100","-",0.63,"-","LCSC",{"$nulls":4},1]
[36,null,"Connector","1 Inner pin IPEX Board-End 1.25mm -40℃~+90℃ 3GHz 50Ω 2mm SMD Coaxial Connectors (RF) ROHS","Shenzhen Kinghelm Elec","KH-IPEX-K501-29",null,null,"J5, J7, J9",3,10,30,null,"SMD",null,"KH-IPEX-K501-29","kinghelm","30","0.0407",1.22,"C411563","LCSC",{"$nulls":4},"J5, J7, J9"]
[37,null,"Connector","NANO SIM+TF /NANO SIM*2","MUP","M6110-01 & M6110-31",null,null,"J6",1,10,10,null,"SMD","Khe cắm và tray Sim",{"$nulls":11},1]
[38,null,"Connector","Card Connector NANO SIM Hinged Lid Surface Mount",null,"C7802-02",null,null,"J23",1,10,10,null,"SMD",null,"C7802-02","MUP","10","0.2735",2.74,"C20624830","LCSC",{"$nulls":4},1]
[39,null,"Connector","67P Surface Mount, Right Angle SMD,P=0.5mm,Surface Mount,Right Angle Centronics Connectors RoHS","FOXCONN","AS0BC21-S40BM-7H",null,null,"J28",1,10,10,null,"SMD",null,"AS0BC21-S40BM-7H","FOXCONN","10","0.3786",3.79,"C410528","LCSC",{"$nulls":4},1]
[40,null,"Crystal","Crystal 27MHz 10ppm 20pF 60Ω SMD2016-4P","MDH","2.D.1.270002002",null,null,"X1",1,10,10,null,"SMD",null,"2.D.1.270002002","MDH","10","0.0479",0.48,"C42420963","LCSC",{"$nulls":4},1]
[41,null,"Diode","DFN1006-2 TVS Diodes ROHS","Leiditech","LM-AZ6118-01F",null,null,"D2, D4, D42, D43",4,10,40,null,"SMD",null,"LM-AZ6118-01F","Leiditech","40","0.0538",2.15,"C49332775","LCSC",{"$nulls":4},"D2,D4"]
[42,null,"Diode","275A 1 Independent 60V 620mV@7A 7A Power-DI-5 Single Diodes RoHS","DIODES","PDS760-13",null,null,"D3",1,10,10,null,"SMD",null,"PDS760-13","DIODES","10","0.3164",3.16,"C96113","LCSC",{"$nulls":4},1]
[43,null,"Diode","Unidirectional 5V (Max) 6.2V 18.6V 9.4A SOD-523 TVS RoHs","Tak cheong","ESD5Z5V0",null,null,"D5, D19, D30",3,10,30,null,"SMD",null,"ESD5Z5V0","MDD(Microdiode Semiconductor)","50","0.0098",0.49,"C502546","LCSC"]
[44,null,"Diode","40V Independent 500mV@3A 3A SMA(DO-214AC) Schottky Diodes ROHS","Guangdong Hottech","SS34A",null,null,"D6",1,10,10,null,"SMD",null,"SS34A","Guangdong Hottech","20","0.0246",0.49,"C2886580","LCSC",{"$nulls":4},1]
[45,null,"Diode","3A@8/20us 23V 70W@8/20us 6V 5V DFN1006-2L TVS Diodes RoHS","Wayon","WE05DGCF-B",null,null,"D7, D35",2,10,20,null,"SMD",null,"WE05DGCF-B","Wayon","20","0.0190",0.38,"C3039401","LCSC"]
[46,null,"Diode","DIODE ZENER 5.1V 500MW SOD123","\tDiodes Incorporated","MMSZ5231B-7-F",null,null,"D8",1,10,10,null,"SMD",null,"MMSZ5231B-7-F","DIODES","20","0.0179",0.36,"C85181","LCSC",{"$nulls":4},1]
[47,null,"Diode","0402 Varistors ROHS","TDK","B72590D50H160",null,null,"D9, D10, D12, D13, D23, D24, D25, D26, D27, D28, D29",11,10,110,null,"SMD",null,"B72590D50H160","TDK","120","0.0165",1.98,"C2842343","LCSC"]
[48,null,"Diode","DIODE GEN PURP 1KV 1A SMA","TDSEMIC","1N4007 M7",null,null,"D20, D47, D48",3,10,30,null,"SMD",null,"-","-",100,"-",0.75,"-","LCSC",{"$nulls":4},"D20"]
[49,null,"Diode","43.6A 9.2V 400W 6.4V Unidirectional 5V SOD-123 TVS Diodes RoHS","FUXINSEMI","PTVS5V0S1UR",null,null,"D39, D40, D41, D44, D45",5,10,50,null,"SMD",null,"PTVS5V0S1UR-MS","MSKSEMI","50","0.0546",2.73,"C30602439","LCSC"]
[50,null,"Diode","Independent Type 10A 1.1V@10A 1kV SMC(DO-214AB) Diodes - General Purpose ROHS","GOODWORK","S10M",null,null,"D52",1,10,10,null,"SMD",null,"S10M","GOODWORK","10","0.0409",0.41,"C2922192","LCSC",{"$nulls":4},1]
[51,null,"Diode","Unidirectional 36V 40V 58.1V 3.4A SOD-123FL TVS RoHS","MDD(Microdiode Semiconductor)","SMF36A",null,null,"D53",1,10,10,null,"SMD",null,"SMF36A","MDD(Microdiode Semiconductor)","20","0.0129",0.26,"C840751","LCSC",{"$nulls":4},1]
[52,null,"Diode","DIODE SCHOTTKY 60V 3A SMAF","HY","SS36F",null,null,"D54, D55",2,10,20,null,"SMD",null,"SS36F","R+O","20","0.0218",0.44,"C41411779","LCSC"]
[53,null,"Ferrite Bead","10mΩ ±25% 10Ω@100MHz 0603 Ferrite Beads and Chips RoHS","YJYCOIN","YI160808U100-5R0T",null,null,"E1, E2, E3, E4, E5, E16, E22, E29, E30, E31, E32",11,10,110,null,"SMD",null,"YI160808U100-5R0T","YJYCOIN","120","0.0156",1.87,"C2971881","LCSC",{"$nulls":4},"E1,E30,E2,E22,e4,e29,e5,e32,e31,e3"]
[54,null,"Ferrite Bead","FERRITE BEAD 1 KOHM 0805 1.5A","Sunlord","UPZ2012E102-1R5TF",null,null,"E6, E15, E26, E27, E28, E33",6,10,60,null,"SMD",null,"XRCB2012U801-1R5TF","XR","100","0.0085",0.85,"C41384122","LCSC",{"$nulls":4},"E6,E33"]
[55,null,"Ferrite Bead","60Ω@100MHz 1 Line Ferrite Bead 0402 600mA 150mΩ","FH","CBW100505U600T",null,null,"E7, E8, E9, E10, E11, E12, E13, E14, E17, E18, E19, E20, E21",13,10,130,null,"SMD",null,"CBW100505U600T","FH","200","0.0019",0.38,"C316432","LCSC"]
[56,null,"IC","2.5MHz Buck Adjustable 800mV~28V 5A SOIC-8-EP Voltage Regulators - DC DC Switching Regulators RoHS","TI","LMR14050SDDAR",null,null,"U1",1,10,10,null,"SMD",null,"LMR14050SDDAR","TI","10","0.3313",3.31,"C155484","LCSC",{"$nulls":4},1]
[57,null,"IC","Buck 1MHz Adjustable 600mV~7.3V 3A SOT23-5 Voltage Regulators - DC DC Switching Regulators RoHS","etasolution","ETA3409S2F",null,null,"U2, U4, U7",3,10,30,null,"SMD",null,"ETA3409S2F","etasolution","30","0.0679",2.04,"C7465553","LCSC",{"$nulls":4},"U2,U7,U4"]
[58,null,"IC","1 Boost VSSOP-10-0.5mm DC DC Switching Controllers RoHS","Texas Instruments","LM3481MMX/NOPB",null,null,"U3",1,10,10,null,"SMD",null,"LM3481MMX/NOPB","TI","10","0.4265",4.2699999999999996,"C543002","LCSC",{"$nulls":4},1]
[59,null,"IC","500mA, low IQ, high precision, adjustable ultra-low dropout voltage regulator with enable function","TI","TLV75801PDBVR",null,null,"U5, U8, U9, U10",4,10,40,null,"SMD",null,"TLV75801PDBVR","TI","40","0.0515",2.06,"C2877852","LCSC",{"$nulls":4},"U5,U8,U9,U10"]
[60,null,"IC","IC DRVR/RCVR MULTCH RS232 16SOIC","Texas Instruments","MAX3232CDR",null,null,"U11, U14, U15",3,10,30,null,"SMD",null,"MAX3232CDR","TI","30","0.2953",8.86,"C45843","LCSC",{"$nulls":4},"U11, U14, U15"]
[{"$f":"ROW(A66)-ROW($A$5)","v":61},null,"IC","LTE CAT 1 module, 4G + (GNSS)","SIMCOM","A7677S",null,null,"U12",1,10,10,null,"SMD",null,"-","-","-","-","-","-","LCSC",{"$nulls":4},1]
[62,null,"IC","SOT-363-6 ESD and Surge Protection (TVS/ESD) ROHS","TECH PUBLIC","SMF05CT1G-P",null,null,"U18",1,10,10,null,"SMD",null,"SMF05CT1G-P","TECH PUBLIC","10","0.0450",0.45,"C2841837","LCSC",{"$nulls":4},1]
[63,null,"IC","SOT-26 ESD and Surge Protection (TVS/ESD) ROHS","Leiditech","SR05-04A",null,null,"U19",1,10,10,null,"SMD",null,"SR05-04A","Leiditech","10","0.0613",0.61,"C5289075","LCSC",{"$nulls":4},1]
[64,null,"IC","2mV 25nA Dual channel SOIC-8 Comparators ROHS","Texas Instruments","LM393DR",null,null,"U21",1,10,10,null,"SMD",null,"LM393DR","TI","10","0.0554",0.55000000000000004,"C67470","LCSC",{"$nulls":4},1]
[65,null,"IC","Costoptimized high performance RX microcontroller with enhanced touch key function and 5V operation support.","Renesas Electronics","R5F51303ADFM",null,null,"U23",1,10,10,null,"SMD",null,"R5F51303ADFM#10","RENESAS","10","2.1177",21.18,"C1018315","LCSC",{"$nulls":4},1]
[66,null,"Inductor","8A 2.2uH ±20% 8.8A 12.5mΩ SMD,7x6.6mm Fixed Inductors RoHS","zoomdo electronics","ZD0650-2R2M",null,null,"L1",1,10,{"$f":"J71*K71","v":10},null,"SMD",null,"ZD0650-2R2M","zoomdo electronics","10","0.0902",0.9,"C48031454","LCSC",{"$nulls":4},1]
[67,null,"Inductor","6A 6.8uH ±20% 39mΩ 10A SMD,7.1x6.6mm Fixed Inductors RoHS","PROD Tech","PSPMAA0605H-6R8M-ANP",null,null,"L2",1,10,10,null,"SMD",null,"PSPMAA0605H-6R8M-ANP","PROD Tech","10","0.1533",1.53,"C2983091","LCSC",{"$nulls":4},1]
[68,null,"Inductor","3.3A 22uH ±20% 7A SMD,12.2x12.2mm Arrays, Signal Transformers RoHS","Sumida","CDRCH12D78BNP-220MC",null,null,"L3",1,10,10,null,"SMD",null,"CDRCH12D78BNP-220MC","Sumida","10","0.6454",6.45,"C2682501","LCSC",{"$nulls":4},1]
[69,null,"Inductor","3.2A 2.2uH 5.8A 34mΩ ±20% SMD,4x4mm Fixed Inductors RoHS","ZE","ZNR3015ST2R2M",null,null,"L4, L5, L6",3,10,30,null,"SMD",null,"ZNR3015ST2R2M","ZE","30","0.0246",0.74,"C42429102","LCSC",{"$nulls":4},"L4,L5,L6"]
[70,null,"Inductor","2A 2.2uH Magnetic Shielded Inductor ±20% 2A 60mΩ SMD,3x3mm Fixed Inductors RoHS","ZE","ZNR3015ST2R2M",null,null,"L7",1,10,10,null,"SMD",null,"ZNR3015ST2R2M","ZE","10","0.0334",0.33,"C42429102","LCSC"]
[71,null,"Inductor","700mA 47nH 160mΩ ±5% 0402 Fixed Inductors RoHS",null,"VHF100505HQ47NJT",null,null,"L8",1,10,10,null,"SMD",null,"VHF100505HQ47NJT","FH","100","0.0018",0.18,"C395068","LCSC"]
[72,null,"Inductor","180mA 68nH ±5% 1.4Ω 0402 Fixed Inductors RoHS","FH","VHF100505HQ68NJT",null,null,"L9",1,10,10,null,"SMD",null,"VHF100505HQ68NJT","FH","100","0.0021",0.21,"C391307","LCSC"]
[73,null,"Inductor","90Ω@100MHz 5Ω 2 SMD-4P,0.8x0.6mm Common Mode Filters ROHS","Murata Electronics","DLM0NSN900HY2D",null,null,"L10",1,10,10,null,"SMD",null,"DLM0NSN900HY2D","muRata","20","0.0203",0.41,"C882594","LCSC"]
[74,null,"LED","20mA 180mcd Colorless Transparent Lens 565nm~575nm -20℃~+85℃ Positive Stick Yellow-green 120° 50mW 2.4V 0603 LED Indication - Discrete ROH","XINGLIGHT","XL-1608SYGC-04",null,null,"D1, D21, D32, D36, D56",5,10,50,null,"SMD",null,"XL-1608SYGC-04","XINGLIGHT","50","0.0055",0.28000000000000003,"C965806","LCSC",{"$nulls":4},"D1"]
[75,null,"LED","20mA 225mcd Colorless Transparent Lens -20℃~+85℃ Positive Stick 620nm~630nm Red 120° 50mW 2.3V 0603 LED Indication - Discrete ROH","XINGLIGHT","XL-1608SURC-06",null,null,"D22, D33",2,10,20,null,"SMD",null,"XL-1608SURC-06","XINGLIGHT","100","0.0019",0.19,"C965799","LCSC"]
[76,null,"LED","LED YELLOW CLEAR 0603 SMD","XINGLIGHT","XL-1608UYC-06","Wurth Electronics Inc,","150060YS75000","D31",1,10,10,null,"SMD",null,"-","-",100,"-",0.7,"-","LCSC"]
[77,null,"IC","GNSS Module with GPS, GLONASS, BDS, Galileo, QZSS, High Sensitivity, Low Power Consumption","SIMCom Wireless Solutions","SIM65M-C",null,null,"M2",1,10,10,null,"SMD",null,"SIM65M","SIMCom Wireless Solutions","10","4.7363",47.36,"C7495025","LCSC",{"$nulls":4},1]
[78,null,"IC","2.5A, 3MHz Switching Charger with Dynamic Power Path Management","etasolution","ETA6003Q3Q",null,null,"U22",1,10,10,null,"SMD",null,"ETA6003Q3Q","etasolution","10","0.2805",2.81,"C5455585","LCSC",{"$nulls":4},1]
[79,null,"MOSFET","N-Channel 30V 0.1A 0.35W Surface Mount SOT-23","JSCJ","2SK3018",null,null,"Q1, Q2, Q5, Q6, Q7, Q8, Q9, Q10, Q11, Q42",10,10,100,null,"SMD",null,"2SK3018","JSCJ","100","0.0125",1.25,"C194460","LCSC",{"$nulls":4},"Q5,Q6,Q7,Q8,Q9,Q10,Q11,Q1,Q2,Q42"]
[80,null,"MOSFET","100V 15A 49mΩ@10V,5A 2.8W 3.2V 1 N-Channel VSONP-8(3.1x3.1) MOSFETs ROHS","Texas Instruments","CSD19538Q3A",null,null,"Q3",1,10,10,null,"SMD",null,"CSD19538Q3A","TI","10","0.2658",2.66,"C478471","LCSC",{"$nulls":4},1]
[81,null,"MOSFET","MOSFET P-CH 30V 4.2A SOT-23","ASDsemi","ASDM3401ZA-R",null,null,"Q13",1,10,10,null,"SMD",null,"ASDM3401ZA-R","ASDsemi","10","0.0380",0.38,"C2758233","LCSC",{"$nulls":4},1]
[82,null,"MOSFET","SOT-23-3 MOSFETs P-Chanel ROHS","TECH PUBLIC","SI2333CDS",null,null,"Q20, Q35, Q36",3,10,30,null,"SMD",null,"SI2333CDS","TECH PUBLIC","30","0.0713",2.14,"C5122040","LCSC"]
[83,null,"MOSFET","50V 200mA 225mW 5.6Ω@2.75V,200mA 500mV 1 N-channel SOT-23 MOSFETs ROHS","LRC","LBSS139LT1G",null,null,"Q22",1,10,10,null,"SMD",null,"LBSS139LT1G","LRC","50","0.0133",0.67,"C383203","LCSC"]
[84,null,"Resistor","RES SMD 1 OHM 1% 1/10W 0603","YAGEO","RC0603FR-071RL",null,null,"R1",1,10,10,null,"SMD",null,"-","-",100,"-",0.38,"-","LCSC",{"$nulls":4},1]
[85,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-07100KL",null,null,"R2, R27, R40, R44, R46, R114, R238, R240, R242",9,10,90,null,"SMD",null,"RC0402FR-07100KL","YAGEO","100","0.0004",0.04,"C60491","LCSC",{"$nulls":4},"R27,R2"]
[86,null,"Resistor","62.5mW 118kΩ 50V Thick Film Resistor ±100ppm/℃ ±0.5% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402DR-07118KL",null,null,"R3",1,10,10,null,"SMD",null,"RC0402DR-07118KL","YAGEO","100","0.0029",0.28999999999999998,"C723573","LCSC",{"$nulls":4},1]
[87,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 68kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0768KL",null,null,"R4",1,10,10,null,"SMD",null,"RC0402FR-0768KL","YAGEO","100","0.0003",0.03,"C137947","LCSC",{"$nulls":4},1]
[88,null,"Resistor","RES 1.1kΩ ±1% 62.5mW 0402","UNI-ROYAL","0402WGF1101TCE",null,null,"R5, R10",2,10,20,null,"SMD",null,"0402WGF1101TCE","UNI-ROYAL","100","0.0004",0.04,"C25860","LCSC",{"$nulls":4},"R5,R10"]
[89,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0710KL",null,null,"R6, R13, R16, R17, R18, R25, R31, R33, R34, R35, R36, R39, R49, R100, R113, R115, R116, R120, R140, R142, R147, R155, R164, R165, R185, R186, R187, R191, R192, R193, R194, R195, R198, R199, R201, R202, R205, R234, R250, R257",40,10,400,null,"SMD",null,"RC0402FR-0710KL","YAGEO","400","0.0004",0.16,"C60490","LCSC",{"$nulls":4},"R13, r16,R25,R18,R250,R33,R257,R6,R34,R35,R164,R165,R17,R49,"]
[90,null,"Resistor","51.1kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-0751K1L",null,null,"R7",1,10,10,null,"SMD",null,"RC0402FR-0751K1L","YAGEO","100","0.0003",0.03,"C327339","LCSC",{"$nulls":4},1]
[91,null,"Resistor","12kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-0712KL",null,null,"R8",1,10,10,null,"SMD",null,"RC0402FR-0712KL","YAGEO","100","0.0004",0.04,"C114760","LCSC",{"$nulls":4},1]
[92,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 1kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-071KL",null,null,"R9, R53, R78, R83, R86, R90, R94, R95, R102, R111, R112, R149, R156, R188, R189, R190, R196, R204, R233, R249, R256, R263",22,10,220,null,"SMD",null,"RC0402FR-071KL","YAGEO","300","0.0004",0.12,"C106235","LCSC",{"$nulls":4},"R256,R9,R53,R78,R83,R86,R90,R102,R94,R95,249,111,112,233,263,149,156,188,196,204,R190,189"]
[93,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 105kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-07105KL",null,null,"R11",1,10,10,null,"SMD",null,"RC0402FR-07105KL","YAGEO","100","0.0004",0.04,"C171671","LCSC",{"$nulls":4},1]
[94,null,"Resistor","52.3kΩ ±1% 62.5mW 0402 Thick Film Resistor","Yageo","RC0402FR-0745K3L",null,null,"R12",1,10,10,null,"SMD",null,"RC0402FR-0745K3L","YAGEO","100","0.0004",0.04,"C137977","LCSC",{"$nulls":4},1]
[95,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 84.5kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0784K5L",null,null,"R14",1,10,10,null,"SMD",null,"RC0402FR-0784K5L","YAGEO","100","0.0001",0.01,"C185390","LCSC",{"$nulls":4},1]
[96,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 100Ω 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-07100RL",null,null,"R15, R104, R105, R152",4,10,40,null,"SMD",null,"RC0402FR-07100RL","YAGEO","100","0.0003",0.03,"C106232","LCSC",{"$nulls":4},"R15"]
[97,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 21.5kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0721K5L",null,null,"R19",1,10,10,null,"SMD",null,"RC0402FR-0721K5L","YAGEO","100","0.0004",0.04,"C185442","LCSC",{"$nulls":4},1]
[98,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 1.91kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-071K91L",null,null,"R20",1,10,10,null,"SMD",null,"RC0402FR-071K91L","YAGEO","100","0.0004",0.04,"C477598","LCSC",{"$nulls":4},1]
[99,null,"Resistor","500mW Thin Film Resistor ±100ppm/℃ ±0.5% 15mΩ 1206 Chip Resistor - Surface Mount ROHS","Yageo","PE1206DRF7W0R015L",null,null,"R21",1,10,10,null,"SMD",null,"PE1206DRF7W0R015L","YAGEO","10","0.1815",1.82,"C1714251","LCSC",{"$nulls":4},1]
[100,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 34kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0734KL",null,null,"R22",1,10,10,null,"SMD",null,"RC0402FR-0734KL","YAGEO","100","0.0004",0.04,"C412507","LCSC",{"$nulls":4},1]
[101,null,"Resistor","45.3kΩ ±1% 62.5mW 0402 Thick Film Resistor","Yageo","RC0402FR-0745K3L",null,null,"R23",1,10,10,null,"SMD",null,"RC0402FR-0745K3L","YAGEO","100","0.0004",0.04,"C137977","LCSC",{"$nulls":4},1]
[102,null,"Resistor","RES SMD 10K OHM 1% 1/10W 0603","Yageo, Hottech","RC0603FR-0710KL, RI0603L1002FT",null,null,"R24, R235",2,10,20,null,"SMD",null,"RC0603FR-0710KL","YAGEO","100","0.0007",7.0000000000000007E-2,"C98220","LCSC",{"$nulls":4},"R24"]
[103,null,"Resistor","62.5mW 499kΩ 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-07499KL",null,null,"R26, R241",2,10,20,null,"SMD",null,"RC0402FR-07499KL","YAGEO","100","0.0004",0.04,"C137971","LCSC",{"$nulls":4},"R26"]
[104,null,"Resistor","8.45kΩ ±1% 62.5mW 0402 Thick Film Resistor","Yageo","RC0402FR-078K45L",null,null,"R29",1,10,10,null,"SMD",null,"RC0402FR-078K45L","YAGEO","100","0.0004",0.04,"C185388","LCSC"]
[105,null,"Resistor","RES SMD 0 OHM JUMPER 1/10W 0603","YAGEO","RC0603JR-070RL",null,null,"R30, R121, R168",3,10,30,null,"SMD",null,"-","-","100","-",0.14000000000000001,"-","LCSC"]
[106,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 2.2kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-072K2L",null,null,"R32, R51, R52, R63, R71, R72, R76, R129, R130, R131, R208, R209, R210, R215, R216, R217, R255, R259",18,10,180,null,"SMD",null,"RC0402FR-072K2L","YAGEO","200","0.0004",0.08,"C114762","LCSC",{"$nulls":4},"R255,R51,R52,R63,R72"]
[107,null,"Resistor","62.5mW Thick Film Resistors 50V ±100ppm/℃ ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-074K7L",null,null,"R37, R38, R45, R64, R73, R80, R96, R97, R103, R134, R135, R141, R144, R148, R206, R211, R213, R218, R220, R221, R244, R251, R254, R260",24,10,240,null,"SMD",null,"RC0402FR-074K7L","YAGEO","300","0.0003",0.09,"C105871","LCSC",{"$nulls":4},"R254, R251,64,73,37,38,45,103,97,260,96,80,134,135,144,244,141,148,206,211,213,218,220,221"]
[108,null,"Resistor","50V Thick Film Resistors 62.5mW 22Ω ±1% ±100ppm/℃ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0722RL",null,null,"R41, R43, R47, R48, R60, R62, R69, R106, R107, R108, R109, R110, R124",13,10,130,null,"SMD",null,"RC0402FR-0722RL","YAGEO","200","0.0003",0.06,"C114765","LCSC",{"$nulls":4},"R47,R48,R41,R43"]
[109,null,"Resistor","62.5mW 1MΩ 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-071ML",null,null,"R42",1,10,10,null,"SMD",null,"RC0402FR-071ML","YAGEO","100","0.0003",0.03,"C138033","LCSC"]
[110,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 15kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0715KL",null,null,"R50, R139",2,10,20,null,"SMD",null,"RC0402FR-0715KL","YAGEO","100","0.0004",0.04,"C114761","LCSC"]
[111,null,"Resistor","62.5mW 4.02Ω 50V Thick Film Resistor ±1% ±200ppm/℃ 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-074R02L",null,null,"R54",1,10,10,null,"SMD",null,"RC0402FR-074R02L","YAGEO","100","0.0012",0.12,"C327249","LCSC"]
[112,null,"Resistor","1.2kΩ ±1% 62.5mW 0402 Thick Film Resistor","Yageo","RC0402FR-071K2L",null,null,"R55",1,10,10,null,"SMD",null,"RC0402FR-071K2L","YAGEO","100","0.0004",0.04,"C138040","LCSC"]
[113,null,"Resistor","62.5mW 0Ω 50V ±1% Thick Film Resistors 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-070RL",null,null,"R56, R57, R58, R59, R61, R65, R66, R67, R68, R70, R74, R75, R98, R99, R119, R138, R154, R157, R246, R247",20,10,200,null,"SMD",null,"RC0402FR-070RL","YAGEO","200","0.0004",0.08,"C106231","LCSC",{"$nulls":4},"R74,R75,R246,R247"]
[114,null,"Resistor","62.5mW Thick Film Resistor 50V ±1% ±200ppm/℃ 10Ω 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0710RL",null,null,"R77, R81, R82, R85, R87, R88, R91, R92, R151, R253",10,10,100,null,"SMD",null,"RC0402FR-0710RL","YAGEO","100","0.0009",0.09,"C138066","LCSC",{"$nulls":4},"77,82,87,91,81,85,88,92,253,151"]
[115,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 75Ω 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0775RL",null,null,"R79, R84, R89, R93",4,10,40,null,"SMD",null,"RC0402FR-0775RL","YAGEO","100","0.0004",0.04,"C114757","LCSC"]
[116,null,"Resistor","220Ω 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-07220RL",null,null,"R101",1,10,10,null,"SMD",null,"RC0402FR-07220RL","YAGEO","100","0.0004",0.04,"C112291","LCSC"]
[117,null,"Resistor","62.5mW 2.2Ω 50V Thick Film Resistor ±1% ±200ppm/℃ 0402 Chip Resistor - Surface Mount RoHS","YAGEO","YAGEO RC0402FR-072R2L",null,null,"R122, R123, R125, R126",4,10,40,null,"SMD",null,"RC0402FR-072R2L","YAGEO","100","0.0008",0.08,"C327251","LCSC"]
[118,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 47kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0747KL",null,null,"R136, R137, R146, R150, R207, R212, R214, R219, R222, R223, R243, R245, R252, R258",14,10,140,null,"SMD",null,"RC0402FR-0747KL","YAGEO","200","0.0003",0.06,"C93943","LCSC",{"$nulls":4},"R252"]
[119,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 470Ω 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-07470RL",null,null,"R163",1,10,10,null,"SMD",null,"RC0402FR-07470RL","YAGEO","100","0.0002",0.02,"C114877","LCSC",{"$nulls":4},1]
[120,null,"Resistor","RES 0 OHM 1206 JUMPER 1/4W SMD","YAGEO","RC1206JR-070RL",null,null,"R166",1,10,10,null,"SMD",null,"-","-","100","-",0.45,"-","LCSC"]
[121,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 20kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0720KL",null,null,"R171",1,10,10,null,"SMD",null,"RC0402FR-0720KL","YAGEO","100","0.0003",0.03,"C93942","LCSC"]
[122,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 590kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","AC0402FR-07590KL",null,null,"R200",1,10,10,null,"SMD",null,"AC0402FR-07590KL","YAGEO","100","0.0006",0.06,"C227149","LCSC"]
[123,null,"Resistor","62.5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 3.3kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-073K3L",null,null,"R203",1,10,10,null,"SMD",null,"RC0402FR-073K3L","YAGEO","100","0.0003",0.03,"C137992","LCSC"]
[124,null,"Resistor","226kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","AC0402FR-07226KL",null,null,"R237",1,10,10,null,"SMD",null,"AC0402FR-07226KL","YAGEO","100","0.0001",0.01,"C226354","LCSC"]
[{"$f":"ROW(A130)-ROW($A$5)","v":125},null,"Resistor","57kΩ 62.5mW 50V Thick Film Resistor ±100ppm/℃ ±1% 0402 Chip Resistor - Surface Mount RoHS","Yageo","RC0402FR-07357KL",null,null,"R239",1,10,10,null,"SMD",null,"RC0402FR-07357KL","YAGEO","100","0.0004",0.04,"C309545","LCSC"]
[126,null,"Switch","Without bracket 50mA 3.5mm 100000 Times 260gf 12V 3mm 2mm Round Button Standing paste SPST SMD Tactile Switches ROHS","XUNPU","TS-1090S-AR02026",null,null,"K1",1,10,10,null,"SMD",null,"TS-1090S-AR02026","XUNPU","10","0.0435",0.44,"C920225","LCSC",{"$nulls":4},1]
[127,null,"Thermistor","10kΩ ±1% 310uA 3435K 100mW ±1% 0603 NTC Thermistors ROHS","Nanjing Shiheng Elec","CMFA 103F3435",null,null,"R236",1,10,10,null,"SMD",null,"CMFA 103F3435","Nanjing Shiheng Elec","20","0.0217",0.43,"C2889048","LCSC"]
[128,null,"Transistor","TRANS NPN 40V 0.2A SOT23","Micro Commercial Co","MMBT3904-TP",null,null,"Q4, Q12, Q16, Q17, Q19, Q21, Q23, Q24, Q25, Q26, Q27, Q28, Q29, Q30, Q31, Q32, Q33, Q34, Q37, Q38, Q39, Q41",22,10,220,null,"SMD",null,"MMBT3904-TP","MCC","250","0.0062",1.55,"C77991","LCSC",{"$nulls":4},"Q4,Q41,Q12,Q34,Q16,Q17, Q39, Q19,Q38,Q37,Q21,Q23,Q26,Q27,Q24,Q25,Q28,Q29,Q30,Q31,Q32,Q33"]
[129,null,"Connector","9P Male D-Sub Bend insert 2 3A -50℃~+105℃ Push-Pull D-Sub / VGA Connectors ROHS","Ckmtw(Shenzhen Cankemeng)","D-DMR009PM-D002",null,null,"J4",1,10,10,null,"TH",null,"D-DMR009PM-D002","Ckmtw","10","0.2550",2.5499999999999998,"C141880","LCSC",{"$nulls":4},1]
[130,null,"Connector","RJ45Receptacle 1 WithLED Plugin Ethernet Connectors / Modular Connectors (RJ45 RJ11) ROHS","HANRUN(Zhongshan HanRun Elec)","HR911105A",null,null,"J10",1,10,{"$f":"J135*K135","v":10},null,"TH",null,"HR911105A","HANRUN(Zhongshan HanRun Elec)","10","1.1989",11.99,"C12074","LCSC",{"$nulls":4},1]
[131,null,"Connector","JUMP-2.0-4PIN-FM-TH",null,"JUMP-2.0-4PIN-FM-TH",null,null,"J11",1,10,10,null,"TH","để hở, không cần connector","-","-","-","-","-","-",{"$nulls":5},1]
[132,null,"Connector","2mm 2mm 2 12P 2x6P -40℃~+105℃ 4.3mm Top 2A Square Hole Through Hole Through Hole,P=2mm Headers, Receptacles, Female Sockets RoHS","XFCN","PM200V-12-12-H43",null,null,"J14, J15, J16",3,10,30,null,"TH",null,"PM200V-12-12-H43","XFCN","35","0.0763",2.67,"C2925565","LCSC",{"$nulls":4},"J14, J15, J16"]
[133,null,"Connector","XH Header Male Pin 0.098\"(2.50mm) 2 Through Hole Wire To Board / Wire To Wire Connector RoHS","BOOMELE(Boom Precision Elec)","XH-2AW",null,null,"J17",1,10,10,null,"TH",null,"XH-2AW","HCTL","50","0.0082",0.41,"C2908611","LCSC",{"$nulls":4},1]
[134,null,"Connector","Pin Header 4 1 Straight，180degrees 2.54mm Through Hole,P=2.54mm Pin Header & Female Header RoHS","CJT(Changjiang Connectors)","A2541WV-4P",null,null,"J24",1,10,10,null,"TH",null,"A2541WV-4P","CJT(Changjiang Connectors)","10","0.0612",0.61,"C5346656","LCSC",{"$nulls":4},1]
[135,null,"Connector","XH Header Male Pin 0.098\"(2.50mm) 2 Through Hole Wire To Board / Wire To Wire Connector RoHS"," \tBOOMELE(Boom Precision Elec)","XH-2A",null,null,"J26",1,10,10,null,"TH",null,"XH-2A","BOOMELE(Boom Precision Elec)","100","0.0054",0.54,"C20079","LCSC",{"$nulls":4},1]
[136,null,"LED","60mA Red Lens 615nm~635nm -20℃~+85℃ Red 50° 150mW 1.8V~2.2V DIP-6-2.54mm LED Indication - Discrete ROHS","XINGLIGHT","XL-DZ304SURD/3",null,null,"LED1, LED2",2,10,20,null,"TH",null,"XL-DZ304SURD/3","XINGLIGHT","20","0.2185",4.37,"C7545656","LCSC"]
[137,null,"Speaker","85dB Active Buzzer (Built-in Driving Circuit) Electromagnetic 3kHz Through Hole,D=9mm Buzzers ROHS","Huaneng","HNB09A05",null,null,"BZ1",1,10,10,null,"TH",null,"HNB09A05","Huaneng","10","0.1934",1.93,"C96493","LCSC"]
[138,null,"Resistor","100mW 0Ω 75V Thick Film Resistor ±5% 0603 Chip Resistor - Surface Mount RoHS","Yageo","RC0603JR-070RL",null,null,"R28",1,10,10,null,"SMD",null,"RC0603JR-070RL","YAGEO","100","0.0006",0.06,"C95177","LCSC",{"$nulls":4},1]
[null,null,"PCB","PCB, 4 layer, 135.1 mm x 134.772 mm, PCB Thickness: 1,56mm, Material Type: FR-4 TG155","JLC",{"$nulls":4},1,10,10,null,"ASM",{"$nulls":7},"JLCPBC"]
[null,null,"Stencil",{"$nulls":6},1,1,1,null,"ASM"]
[{"$nulls":4},"TỔNG",{"$nulls":14},{"$f":"SUM(T6:T145)","v":194.02999999999989}]

{"sheet":"GX Board","index":1,"n_rows":18,"n_cols":21,"rows_kept":18,"cut":false,"hidden":false,"merged":[[3,0,3,1],[3,9,3,14],[1,17,1,19],[2,17,2,19],[0,0,1,2],[0,3,0,8],[0,9,0,13],[1,3,1,8],[1,9,1,13],[2,0,2,1],[2,9,2,14]]}
[null,null,null,{"$f":"UPPER(\"Bill of Materials\")","v":"BILL OF MATERIALS"},{"$nulls":5},"Rev:"]
[null,null,null,"Camera_box_gx",{"$nulls":5},"Production QTY",{"$nulls":7},"BOM Export Date: 04/05/26 16:31:42"]
["Customer:",null,"Aithings","HW version:","5.0",null,"Checked by:",null,null,"Date created:",{"$nulls":7},"Website：https://www,lcsc,com/bom"]
["Board code:",null,"Camera_box_gx","Prepared by:","Ducdv",null,"Approved by:",null,null,"26/03/2026"]
["STT","Internal Code","Category","Description","Manufacture","Partnumber","Manufacturer 2","Manufacturer's Part Number 2","Designator","Quantity","Board","Total","Unit","Mounting type","Note","Order Qty.","Unit Price(USD)","Ext,Price(USD)","LCSC#","Package"]
[{"$f":"ROW(A6)-ROW($A$5)","v":1},null,"Capacitor","CAP CER 1UF 50V X5R 0603",null,null,"Samsung Electro-Mechanics","CL10A105KB8NNNC","C1, C2, C3, C4",4,10,{"$f":"J6*K6","v":40},null,"SMD",null,50,"-",0.39,"-","-"]
[2,null,"Connector","2x2P 4P Micro-Fit(MX 3,0) 3mm 2 2 3mm Direct Insert Plugin,P=3mm Wire To Board Connector ROHS","BOOMELE(Boom Precision Elec)","3,0-2*2A",null,null,"J7, J9, J10, J11, J12, J13",6,10,{"$f":"J7*K7","v":60},null,"SMD",null,"60","0.0637",3.82,"C173283","-"]
[3,null,"Connector","2x6P 12P Gold Brass -40℃~+105℃ Pin Header Black 2mm 2mm 250V 3A 2 2mm SMD,P=2mm Headers, Male Pins ROHS","XKB Connection","X4621WRS-2x06I-C40D64","XKB Connection","X4621WRS-2x03I-C40D64","J8, J14, J15",3,10,30,null,"SMD",null,"30","0.2929",8.7899999999999991,"C5242507","-"]
[4,null,"MOSFET","SOT-23-3 MOSFETs P-Chanel ROHS","TECH PUBLIC","SI2333CDS",null,null,"Q1, Q2, Q5, Q6",4,10,40,null,"SMD",null,"40","0.0711",2.84,"C5122040","-"]
[5,null,"Resistor","62,5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0710KL",null,null,"R1, R2, R7, R8",4,10,40,null,"SMD",null,"100","0.0004",0.04,"C60490","-"]
[6,null,"Resistor","62,5mW Thick Film Resistors 50V ±100ppm/℃ ±1% 4,7kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-074K7L",null,null,"R3, R4, R9, R10",4,10,40,null,"SMD",null,"100","0.0003",0.03,"C105871","-"]
[7,null,"Resistor","62,5mW Thick Film Resistor 50V ±100ppm/℃ ±1% 47kΩ 0402 Chip Resistor - Surface Mount ROHS","Yageo","RC0402FR-0747KL",null,null,"R5, R6, R11, R12",4,10,40,null,"SMD",null,"100","0.0003",0.03,"C93943","-"]
[8,null,"Transistor","TRANS NPN 60V 0,5A SOT23","ON Semiconductor","MMBTA05LT1G",null,null,"Q3, Q4, Q7, Q8",4,10,40,null,"SMD",null,"40","0.0276",1.1000000000000001,"C152279","-"]
[9,null,"Connector","Giắc GX12-2P 2 Chân (Đực)","LKTC","GX12-2P",null,null,"J1",1,10,10,null,"TH",null,"10","1.2344",12.34,"C18203260","-"]
[10,null,"Connector","Giắc GX12-4P 12mm 4 Chân (Đực)","LKTC","GX12-4P",null,null,"J2, J3, J5, J6",4,10,40,null,"TH",null,"40","1.2998",51.99,"C18203262","-"]
[11,null,"PCB","PCB, 2 layer, 113,94 mm* 23,58 mm, PCB Thickness: 1,6mm, Gerber_Camerabox-gx_2025-11-24_Y2413","JLC","Y2413",null,null,null,1,10,10,null,"ASM",null,"-","-","-","-","-"]
[12,null,"Stencil",{"$nulls":6},1,10,10,null,"ASM",null,"-","-","-","-","-"]
[null,null,null,"TỔNG",{"$nulls":13},{"$f":"SUM(R6:R17)","v":81.37},null,null,"USD"]

{"sheet":"Vat_tu_phu","index":2,"n_rows":16,"n_cols":20,"rows_kept":16,"cut":false,"hidden":false,"merged":[[1,15,1,18],[3,0,3,1],[3,9,3,14],[0,0,1,2],[0,3,0,8],[0,9,0,13],[1,3,1,8],[1,9,1,13],[2,0,2,1],[2,9,2,14]]}
[null,null,null,{"$f":"UPPER(\"Bill of Materials\")","v":"BILL OF MATERIALS"},{"$nulls":5},"Rev:"]
[null,null,null,"Camera_box_vật tư phụ",{"$nulls":5},"Production QTY",{"$nulls":5},"Nguồn khác"]
["Customer:",null,"Aithings","HW version:","5.0",null,"Checked by:",null,null,"Date created:"]
["Board code:",null,"Vật tư phụ","Prepared by:","Ducdv",null,"Approved by:",null,null,"26/03/2026"]
["STT","Internal Code","Category","Description","Manufacture","Partnumber","Manufacturer 2","Manufacturer's Part Number 2","Designator","Quantity/kit","Board","Total","Unit","Mounting type","Note","Order Qty.","Unit Price(VND)","Ext,Price(VND)","Nguồn"]
[{"$f":"ROW(A6)-ROW($A$5)","v":1},null,"Battery","Pin Lithium","Shoppe: AM Linh Kiện",{"$nulls":4},1,10,{"$f":"J6*K6","v":10},null,"ASM",null,10,50000,{"$f":"Q6*P6","v":500000},"https://shopee.vn/product/472471748/27209001295?gads_t_sig=gqRjZGVrxHCFomtpsTE0MjUxOnRzc19zZGtfa2V5omt20QABpGFsZ2_SAAAAZKNkZWvAomN0xEAAAAAMRoz0ZUjQw0QlRa--FjB0AKnHQPF7xv4DyGj9-GQwqn4zSdB6gztmw7ebmtsZs9FPJxlVqctc57WUE3IRqmNpcGhlcnRleHTEbgAAAAzOmWiKQhTD73oy3pMTD74YwXKLY4RmTmx_PECgQdqrSMko9Yj-LV50FldCrrJu5kPHupxjQruBx93-Rht53dteckDz3PQ9R9Ffxg1CnUg0Q4ADNZT7dVO_ek6XNMjV98hEJY0-rMFUz31c&gad_source=1&gad_campaignid=22506035722&gbraid=0AAAAADPpQE6U2mKiUDG5SpqIjApCVJLCa&gclid=Cj0KCQjwh-HPBhCIARIsAC0p3ccvrmVkDpuOBH77KWqu0VKbvpR57SbJKexkpAHzM0uqhK1QMQfLJz4aAmzGEALw_wcB"]
[2,null,"BOX","Vỏ hộp ","Kadotech","KDT-2526",null,null,null,1,10,10,null,"ASM",null,"-",null,"-","Chưa tìm được nguồn mua phù hợp"]
[3,null,"Connector","Cáp RF Đầu SMA Cái Nối 1,13Ipex Dài 10cm","TGIC","1,13Ipex",null,null,null,2,10,20,null,"ASM",null,20,11970,{"$f":"Q8*P8","v":239400},"https://www.thegioiic.com/cap-rf-dau-sma-cai-noi-1-13ipex-dai-10cm"]
[4,null,"Product","Miếng dẫn nhiệt thermal pad 5W/mK cho vga, chipset, ic dày 0,5, 1, 1,5, 2, 2,5, 3, 5mm ,kienstore358","Shopee\nkienstore358","100x100x2mm",null,null,null,1,5,5,null,"ASM","Tản nhiệt SOM",3,46500,{"$f":"Q9*P9","v":139500},"https://shopee.vn/product/16195091/3632842107?gads_t_sig=gqRjZGVrxHCFomtpsTE0MjUxOnRzc19zZGtfa2V5omt20QABpGFsZ2_SAAAAZKNkZWvAomN0xEAAAAAMRoz0ZUjQw0QlRa--FjB0AKnHQPF7xv4DyGj9-GQwqn4zSdB6gztmw7ebmtsZs9FPJxlVqctc57WUE3IRqmNpcGhlcnRleHTEagAAAAxLgiQivYZgW5foBPUBW12V8NHF09EY7qvmQOS38IA2e0CYjRekDsolqv8LMehX3QA7bJdvA0ZGP-sAncSvKGxwbMeXwQx2NGhEZXdYRNYdiWPk82HQPWPYfVW33Sbu0RV7orG3wGk&gad_source=1&gad_campaignid=22496000355&gbraid=0AAAAADPpQE6bBolz_JwwPGJCnXnPJllEZ&gclid=Cj0KCQjwh-HPBhCIARIsAC0p3ccJjJk5KYxemJ07EzcLDLZYWXACEOCjEViEVKBJMcyI0qedliT716YaAkxiEALw_wcB"]
[5,null,"Quạt","Quạt Tản Nhiệt Mini 2510 – Quạt 2.5cm 25x25x10mm 5V / 12V DC – Gió Mạnh, Nhỏ Gọn, Ít Tiếng Ồn","SHOPPE","Mini Eibbkg 5V",null,null,null,1,10,10,null,"ASM",null,10,35000,{"$f":"Q10*P10","v":350000},"https://shopee.vn/Qu%EF%BF%BD%E1%BA%A1t-T%E1%BA%A3n-Nhi%E1%BB%87t-Mini-2510-%E2%80%93-Qu%E1%BA%A1t-2.5cm-25x25x10mm-5V-12V-DC-%E2%80%93-Gi%C3%B3-M%E1%BA%A1nh-Nh%E1%BB%8F-G%E1%BB%8Dn-%C3%8Dt-Ti%E1%BA%BFng-%E1%BB%92n-i.983524123.51300841631?extraParams=%7B%22display_model_id%22%3A445075556373%2C%22model_selection_logic%22%3A3%7D"]
[6,null,"Screw","10 cái M3 M4 M5 Bulong lục giác chìm đầu bằng đen thép mạ cấp bền 10,9 M3 M4 M5","Shopee Khôi Fasten","M3x16mm",null,null,null,4,10,40,null,"ASM","Vít cho quạt",50,{"$f":"35000/50","v":700},{"$f":"Q11*P11","v":35000},"https://shopee.vn/50-c%C3%A1i-M3-M4-M5-Bulong-l%E1%BB%A5c-gi%C3%A1c-ch%C3%ACm-%C4%91%E1%BA%A7u-b%E1%BA%B1ng-%C4%91en-th%C3%A9p-m%E1%BA%A1-c%E1%BA%A5p-b%E1%BB%81n-10.9-i.39096692.12657476490"]
[7,null,"Screw","Set 50, 20 Tán Dẹp Ecu Inox 304, thép thôi, thép mạ Cho ốc M3, M4, M5, M6, M8 Set 10 con đai ốc inox loại tốt","Linh kiện điện tử SMD","M3 Inox304",null,null,null,4,10,40,null,"ASM","Bulong hàn cho quạt",50,1600,{"$f":"Q12*P12","v":80000},"https://shopee.vn/product/134796651/18762050701?gads_t_sig=gqRjZGVrxHCFomtpsTE0MjUxOnRzc19zZGtfa2V5omt20QABpGFsZ2_SAAAAZKNkZWvAomN0xEAAAAAMRoz0ZUjQw0QlRa--FjB0AKnHQPF7xv4DyGj9-GQwqn4zSdB6gztmw7ebmtsZs9FPJxlVqctc57WUE3IRqmNpcGhlcnRleHTEbgAAAAyjVrs0gr8UnuryeetI3FX5Y16AmL_mbFh-BhzhNYSPCYip1w6WS6FoDljuqhTt2G5b1K_wR9XnDLR9WZzE5wC81X4yviPtEfAPixm0EH_uhDsW8r7vXboffenME-Yw3AOA9ysYlFQUXDIh&gad_source=1&gad_campaignid=22496000355&gbraid=0AAAAADPpQE6bBolz_JwwPGJCnXnPJllEZ&gclid=Cj0KCQjwh-HPBhCIARIsAC0p3cfnu3W1ldu4Fhpn7GV8qDwtxFhI1ARvfrlSmeh8cJ9jHKLEj-Gj6C4aAurrEALw_wcB"]
[8,null,"Screw","M1,2 M1,4 M1,6 M2 M2,5 M3 M4 M5 M6 Thép Carbon Kẽm Đen CM Cross Phillips Siêu Mỏng Siêu Thấp Đầu Phẳng Vít Bu Lông","Shopee huiruixin,vn","M1,4x2,5mm",null,null,null,1,10,10,null,"ASM","Vít cho SOM",500,null,52000,"https://shopee.vn/M1.2-M1.4-M1.6-M2-M2.5-M3-M4-M5-M6-Th%C3%A9p-Carbon-K%E1%BA%BDm-%C4%90en-CM-Cross-Phillips-Si%C3%AAu-M%E1%BB%8Fng-Si%C3%AAu-Th%E1%BA%A5p-%C4%90%E1%BA%A7u-Ph%E1%BA%B3ng-V%C3%ADt-Bu-L%C3%B4ng-i.889466159.28555773016?extraParams=%7B%22display_model_id%22%3A246227873566%2C%22model_selection_logic%22%3A3%7D"]
[9,null,"Screw","Bộ 10 Long đen/ vòng đệm các kích thước.M1.6 M2 M2.5 M3 M4 M6 M8 M10 M12 M14","Linh kiện điện tử SMD","M3",null,null,null,4,10,40,null,"ASM","Vênh cho quạt",40,null,20000,"https://shopee.vn/product/51517981/5019789812?gads_t_sig=gqRjZGVrxHCFomtpsTE0MjUxOnRzc19zZGtfa2V5omt20QABpGFsZ2_SAAAAZKNkZWvAomN0xEAAAAAMRoz0ZUjQw0QlRa--FjB0AKnHQPF7xv4DyGj9-GQwqn4zSdB6gztmw7ebmtsZs9FPJxlVqctc57WUE3IRqmNpcGhlcnRleHTEagAAAAyUnapXmxqrtAARC2f2cAyv2rWo4S6nSmJarRu2hF963X_eLnWICFmDLSksVdDtVkHlcvDes5vsZPttikVHhlfJAtwmGUBR9F0tm60UZ4rTVfZJAH2dWM_Bkpq7YSLuwi3vIB1wnUw&gad_source=1&gad_campaignid=22651004374&gbraid=0AAAAADPpQE6hA2b-beNyuq8-eNHxmjDX-&gclid=Cj0KCQjwh-HPBhCIARIsAC0p3ceXFYtQJC6HCGelD_ac7vc2P3AYvNRl1mFwCvvVQZLvehYiAS0tv8saAhFLEALw_wcB"]
[10,null,"Connector","Giắc GX12-2P 2 Chân (Cái) Đấu Dây Test","LKTC","GX12-2P (Cái)",null,null,null,1,10,10,null,"ASM",null,10,6200,{"$f":"Q15*P15","v":62000},"https://www.thegioiic.com/gx12-2p-dau-noi-tron-cai-2-chan-thang-hang-3a-125v"]
[null,null,null,"TỔNG",{"$nulls":13},{"$f":" SUM(R6:R15)","v":1477900},null,"VND"]

{"sheet":"Chi phí","index":3,"n_rows":4,"n_cols":8,"rows_kept":4,"cut":false,"hidden":false,"merged":[[1,6,3,6]]}
["STT","Loại","Số lượng","Đơn giá","Đơn vị","Quy đổi(VND)","Tổng tiền (VND)","Ghi chú"]
[1,"RV1106 Board",1,{"$f":"RV1106_Board!T146","v":194.02999999999989},"USD",{"$f":"D2*26337","v":5110168.1099999966},{"$f":"F2+F3+F4","v":8731109.799999997}]
[2,"Vat_tu_phu",1,{"$f":"Vat_tu_phu!R16","v":1477900},"VND",{"$f":"D3","v":1477900}]
[3,"GX_Board",1,{"$f":"'GX Board'!$R$18","v":81.37},"USD",{"$f":"D4*26337","v":2143041.69}]